#!/sbin/openrc-run
# Copyright 1999-2013 Gentoo Foundation
# Distributed under the terms of the GNU General Public License, v2 or later
# $Header: /var/cvsroot/gentoo-x86/sys-cluster/drbd/files/drbd-8.0.rc,v 1.8 2013/01/17 19:09:04 robbat2 Exp $

extra_started_commands="reload"

depend() {
	use logger
	need net
	before heartbeat
	after sshd
}

DEFAULTFILE="/etc/conf.d/drbd"
DRBDADM="/sbin/drbdadm"
PROC_DRBD="/proc/drbd"
MODPROBE="/sbin/modprobe"
RMMOD="/sbin/rmmod"
UDEV_TIMEOUT=10
ADD_MOD_PARAM=""

if [ -f $DEFAULTFILE ]; then
  . $DEFAULTFILE
fi

# Just in case drbdadm want to display any errors in the configuration
# file, or we need to ask the user about registering this installation
# at http://usage.drbd.org, we call drbdadm here without any IO
# redirection.
$DRBDADM sh-nop

assure_module_is_loaded() {
	[ -e "$PROC_DRBD" ] && return
	ebegin "Loading drbd module"
	ret=0

	$MODPROBE -s drbd `$DRBDADM sh-mod-parms` $ADD_MOD_PARAM || ret=20
	eend $ret
	return $ret
}

adjust_with_progress() {
	IFS_O=$IFS
	NEWLINE='
'
	IFS=$NEWLINE
	local D=0
	local S=0
	local N=0

	einfon "Setting drbd parameters "
	COMMANDS=`$DRBDADM -d adjust all` || {
		eend 20 "Error executing drbdadm"
		return 20
	}
	echo -n "[ "

	for CMD in $COMMANDS; do
		if echo $CMD | grep -q disk; then echo -n "d$D "; D=$(( D+1 ));
		elif echo $CMD | grep -q syncer; then echo -n "s$S "; S=$(( S+1 ));
		elif echo $CMD | grep -q net; then echo -n "n$N "; N=$(( N+1 ));
		else echo -n ".. ";
		fi
		IFS=$IFS_O
		$CMD || {
			echo
			eend 20 "cmd $CMD failed!"
			return 20
		}
		IFS=$NEWLINE
	done
	echo "]"
	eend 0

	IFS=$IFS_O
}

start() {
	einfo "Starting DRBD resources:"
	eindent
	assure_module_is_loaded || return $?
	adjust_with_progress || return $?

	# make sure udev has time to create the device files
	ebegin "Waiting for udev device creation ..."
	for RESOURCE in `$DRBDADM sh-resources`; do
		for DEVICE in `$DRBDADM sh-dev $RESOURCE`; do
			UDEV_TIMEOUT_LOCAL=$UDEV_TIMEOUT
			while [ ! -e $DEVICE ] && [ $UDEV_TIMEOUT_LOCAL -gt 0 ] ; do
				sleep 1
				UDEV_TIMEOUT_LOCAL=$(( $UDEV_TIMEOUT_LOCAL-1 ))
			done
		done
	done
	eend 0

	einfon "Waiting for connection "
	$DRBDADM wait-con-int
	ret=$?
	echo

	sleep 5

	einfon "Become primary if configured "
	$DRBDADM sh-b-pri all
	echo

	eend $ret
	return $ret
}

stop() {
	ebegin "Stopping all DRBD resources"

	# Check for mounted drbd devices
	if ! grep -q '^/dev/drbd' /proc/mounts &>/dev/null; then
		if [ -e ${PROC_DRBD} ]; then
			${DRBDADM} down all
			ret=$?
			sleep 3
			if [ -e /proc/modules ] && grep -q '^drbd' /proc/modules ; then
			      ${RMMOD} drbd
			fi
		fi
		eend $ret
		return $ret
	else
		einfo "drbd devices mounted, please umount them before trying to stop drbd!"
		eend 1
		return 1
	fi
}

status() {
	# NEEDS to be heartbeat friendly...
	# so: put some "OK" in the output.

	if [ -e $PROC_DRBD ]; then
		ret=0
		ebegin "drbd driver loaded OK; device status:"
		eend $ret
		cat $PROC_DRBD
	else
		ebegin "drbd not loaded"
		ret=3
		eend $ret
	fi
	return $ret
}

reload() {
	ebegin "Reloading DRBD"
	${DRBDADM} adjust all
	ret=$?
	eend $ret
	return $ret
}
