#!/sbin/openrc-run

description="A lightweight DNS, DHCP, RA, TFTP and PXE server"

extra_commands="checkconfig"
description_checkconfig="Check configuration syntax"

extra_started_commands="reload"
description_reload="Clear cache and reload hosts files"

: ${DNSMASQ_CONFFILE:=/etc/dnsmasq.conf}

command="/usr/sbin/dnsmasq"
# Tell dnsmasq to not create pidfile, that's responsibility of init system.
command_args="-k --pid-file= $DNSMASQ_OPTS --conf-file=$DNSMASQ_CONFFILE"
command_background="yes"
pidfile="/run/${RC_SVCNAME}.pid"
leasefile=/var/lib/misc/$RC_SVCNAME.leases

if [ "${RC_SVCNAME#*.}" != "$RC_SVCNAME" ]; then
	BRIDGE="${RC_SVCNAME#*.}"
	: ${BRIDGE_ADDR:="10.0.3.1"}
	: ${BRIDGE_NETMASK:="255.255.255.0"}
	: ${BRIDGE_NETWORK:="10.0.3.0/24"}
	: ${BRIDGE_DHCP_RANGE:="10.0.3.2,10.0.3.254"}
	: ${BRIDGE_DHCP_MAX:="253"}
	: ${BRIDGE_MAC:="00:16:3e:00:00:00" }
fi
.

depend() {
	provide dns
	need localmount net
	after bootmisc
	use logger
}

setup_firewall() {
	local ins=$1 add=$2
	iptables -w $ins INPUT -i ${BRIDGE} -p udp --dport 67 -j ACCEPT
	iptables -w $ins INPUT -i ${BRIDGE} -p tcp --dport 67 -j ACCEPT
	iptables -w $ins INPUT -i ${BRIDGE} -p udp --dport 53 -j ACCEPT
	iptables -w $ins INPUT -i ${BRIDGE} -p tcp --dport 53 -j ACCEPT
	iptables -w $ins FORWARD -i ${BRIDGE} -j ACCEPT
	iptables -w $ins FORWARD -o ${BRIDGE} -j ACCEPT
	iptables -w -t nat $add POSTROUTING -s ${BRIDGE_NETWORK} ! -d ${BRIDGE_NETWORK} -j MASQUERADE
	iptables -w -t mangle $add POSTROUTING -o ${BRIDGE} -p udp -m udp --dport 68 -j CHECKSUM --checksum-fill
}

setup_bridge() {
	if ! [ -d /sys/class/net/$BRIDGE ]; then
		ip link add dev $BRIDGE type bridge
	fi
	ip addr add ${BRIDGE_ADDR}/${BRIDGE_NETMASK} dev $BRIDGE \
		&& ip link set dev $BRIDGE address ${BRIDGE_MAC} \
		&& ip link set dev $BRIDGE up

	 echo 1 > /proc/sys/net/ipv4/ip_forward
	 echo 0 > /proc/sys/net/ipv6/conf/${BRIDGE}/accept_dad || true

	if [ -n "$BRIDGE_IPV6_ADDR" ] && [ -n "$BRIDGE_IPV6_MASK" ] && [ "$BRIDGE_IPV6_NETWORK" ]; then
		echo 1 > /proc/sys/net/ipv6/conf/all/forwarding
		echo 0 > /proc/sys/net/ipv6/conf/${BRIDGE}/autoconf
		ip -6 addr add dev ${BRIDGE} ${BRIDGE_IPV6_ADDR}/${BRIDGE_IPV6_MASK}
		if [ "$BRIDGE_IPV6_NAT" = "true" ]; then
			ip6tables -w -t nat -A POSTROUTING -s ${BRIDGE_IPV6_NETWORK} ! -d ${BRIDGE_IPV6_NETWORK} -j MASQUERADE
		fi
		command_args="$command_args --dhcp-range=${BRIDGE_IPV6_ADDR},ra-only --listen-address ${BRIDGE_IPV6_ADDR}"
	fi

}

start_pre() {
	$command --test --conf-file=$DNSMASQ_CONFFILE >/dev/null 2>&1 \
		|| $command --test || return 1
	checkpath -m 0644 -o dnsmasq:dnsmasq -f $leasefile || return 1

	if [ -n "$DNSMASQ_CONFFILE" ]; then
		command_args="$command_args --conf-file=$DNSMASQ_CONFFILE"
	fi
	if [ -z "$BRIDGE" ]; then
		return 0
	fi

	setup_bridge
	if [ -z "$DISABLE_IPTABLES" ]; then
		setup_firewall -I -A
	fi
	command_args="$command_args --strict-order --bind-interfaces --listen-address ${BRIDGE_ADDR} --except-interface=lo --interface=$BRIDGE --dhcp-range $BRIDGE_DHCP_RANGE --dhcp-lease-max=$BRIDGE_DHCP_MAX --dhcp-no-override --dhcp-leasefile=$leasefile --dhcp-authoritative"
}

stop_post() {
	if [ -n "$BRIDGE" ]; then
		ip addr del ${BRIDGE_ADDR}/${BRIDGE_NETMASK} dev $BRIDGE
		ip link set dev $BRIDGE down
		if [ -z "$DISABLE_IPTABLES" ]; then
			setup_firewall -D -D
		fi
		# dont destroy if there are attached interfaces
		ls /sys/class/net/${BRIDGE}/brif/* > /dev/null 2>&1 || ip link delete ${BRIDGE}
	fi
}

reload() {
	ebegin "Reloading $RC_SVCNAME"
	$command --test --conf-file=$DNSMASQ_CONFFILE >/dev/null 2>&1 \
		|| $command --test || return 1
	start-stop-daemon --signal HUP --pidfile "$pidfile"
	eend $?
}

checkconfig() {
	ebegin "Checking $RC_SVCNAME configuration"
	$command --test --conf-file=$DNSMAQ_CONFFILE
	eend $?
}
