From 2c82524000cca691c89c9fda251b55ef04eabcb6 Mon Sep 17 00:00:00 2001
From: Mathias Kresin <openwrt@kresin.me>
Date: Mon, 2 May 2016 18:50:00 +0000
Subject: [PATCH] find active root

Signed-off-by: Mathias Kresin <openwrt@kresin.me>
---
 drivers/mtd/parsers/ofpart_core.c | 49 ++++++++++++++++++++++++++++++-
 1 file changed, 48 insertions(+), 1 deletion(-)

--- a/drivers/mtd/parsers/ofpart_core.c
+++ b/drivers/mtd/parsers/ofpart_core.c
@@ -38,6 +38,38 @@ static bool node_has_compatible(struct d
 	return of_get_property(pp, "compatible", NULL);
 }
 
+static uint8_t * brnboot_get_selected_root_part(struct mtd_info *master,
+						loff_t offset)
+{
+	static uint8_t root_id;
+	int err, len;
+
+	err = mtd_read(master, offset, 0x01, &len, &root_id);
+
+	if (mtd_is_bitflip(err) || !err)
+		return &root_id;
+
+	return NULL;
+}
+
+static void brnboot_set_active_root_part(struct mtd_partition *pparts,
+					 struct device_node **part_nodes,
+					 int nr_parts,
+					 uint8_t *root_id)
+{
+	int i;
+
+	for (i = 0; i < nr_parts; i++) {
+		int part_root_id;
+
+		if (!of_property_read_u32(part_nodes[i], "brnboot,root-id", &part_root_id)
+		    && part_root_id == *root_id) {
+			pparts[i].name = "firmware";
+			break;
+		}
+	}
+}
+
 static int parse_fixed_partitions(struct mtd_info *master,
 				  const struct mtd_partition **pparts,
 				  struct mtd_part_parser_data *data)
@@ -51,6 +83,8 @@ static int parse_fixed_partitions(struct
 	struct device_node *pp;
 	int nr_parts, i, ret = 0;
 	bool dedicated = true;
+	uint8_t *proot_id = NULL;
+	struct device_node **part_nodes;
 
 	/* Pull of_node from the master device node */
 	mtd_node = mtd_get_of_node(master);
@@ -95,7 +129,9 @@ static int parse_fixed_partitions(struct
 		return 0;
 
 	parts = kcalloc(nr_parts, sizeof(*parts), GFP_KERNEL);
-	if (!parts)
+	part_nodes = kcalloc(nr_parts, sizeof(*part_nodes), GFP_KERNEL);
+
+	if (!parts || !part_nodes)
 		return -ENOMEM;
 
 	i = 0;
@@ -166,6 +202,11 @@ static int parse_fixed_partitions(struct
 		if (of_property_read_bool(pp, "slc-mode"))
 			parts[i].add_flags |= MTD_SLC_ON_MLC_EMULATION;
 
+		if (!proot_id && of_device_is_compatible(pp, "brnboot,root-selector"))
+			proot_id = brnboot_get_selected_root_part(master, parts[i].offset);
+
+		part_nodes[i] = pp;
+
 		i++;
 	}
 
@@ -175,6 +216,11 @@ static int parse_fixed_partitions(struct
 	if (quirks && quirks->post_parse)
 		quirks->post_parse(master, parts, nr_parts);
 
+	if (proot_id)
+		brnboot_set_active_root_part(parts, part_nodes, nr_parts, proot_id);
+
+	kfree(part_nodes);
+
 	*pparts = parts;
 	return nr_parts;
 
@@ -185,6 +231,7 @@ ofpart_fail:
 ofpart_none:
 	of_node_put(pp);
 	kfree(parts);
+	kfree(part_nodes);
 	return ret;
 }
 
