From: Felix Fietkau <nbd@nbd.name>
Date: Fri, 6 May 2022 21:38:42 +0200
Subject: [PATCH] net: dsa: tag_mtk: add padding for tx packets

Padding for transmitted packets needs to account for the special tag.
With not enough padding, garbage bytes are inserted by the switch at the
end of small packets.

Fixes: 5cd8985a1909 ("net-next: dsa: add Mediatek tag RX/TX handler")
Signed-off-by: Felix Fietkau <nbd@nbd.name>
---

--- a/net/dsa/tag_mtk.c
+++ b/net/dsa/tag_mtk.c
@@ -29,6 +29,13 @@ static struct sk_buff *mtk_tag_xmit(stru
 
 	skb_set_queue_mapping(skb, dp->index);
 
+	/* The Ethernet switch we are interfaced with needs packets to be at
+	 * least 64 bytes (including FCS) otherwise their padding might be
+	 * corrupted. With tags enabled, we need to make sure that packets are
+	 * at least 68 bytes (including FCS and tag).
+	 */
+	eth_skb_pad(skb);
+
 	/* Build the special tag after the MAC Source Address. If VLAN header
 	 * is present, it's required that VLAN header and special tag is
 	 * being combined. Only in this way we can allow the switch can parse
