From b6764bb27c819cdcf854371db485a43d71f579f3 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Petr=20=C5=A0tetiar?= <ynezz@true.cz>
Date: Tue, 3 Mar 2020 15:15:57 +0100
Subject: [PATCH] ARM: dts: imx6q-apalis: ixora: make switch3 reset button
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Petr Štetiar <ynezz@true.cz>
---
 arch/arm/boot/dts/nxp/imx/imx6q-apalis-ixora-v1.1.dts | 15 ++++++++++++++-
 arch/arm/boot/dts/nxp/imx/imx6q-apalis-ixora.dts      | 15 ++++++++++++++-
 2 files changed, 28 insertions(+), 2 deletions(-)

--- a/arch/arm/boot/dts/nxp/imx/imx6q-apalis-ixora.dts
+++ b/arch/arm/boot/dts/nxp/imx/imx6q-apalis-ixora.dts
@@ -59,6 +59,17 @@
 			label = "LED_5_RED";
 		};
 	};
+
+	gpio-keys {
+		pinctrl-0 = <&pinctrl_gpio_keys &pinctrl_switch3_ixora>;
+
+		reset {
+			label = "reset";
+			gpios = <&gpio1 16 GPIO_ACTIVE_LOW>;
+			linux,code = <KEY_RESTART>;
+			debounce-interval = <10>;
+		};
+	};
 };
 
 &can1 {
@@ -183,4 +194,10 @@
 			MX6QDL_PAD_NANDF_D2__GPIO2_IO02 0x1b0b0
 		>;
 	};
+
+	pinctrl_switch3_ixora: switch3ixora {
+		fsl,pins = <
+			MX6QDL_PAD_SD1_DAT0__GPIO1_IO16 0x1b0b0
+		>;
+	};
 };
--- a/arch/arm/boot/dts/nxp/imx/imx6q-apalis-ixora-v1.2.dts
+++ b/arch/arm/boot/dts/nxp/imx/imx6q-apalis-ixora-v1.2.dts
@@ -61,6 +61,17 @@
 		};
 	};
 
+	gpio-keys {
+		pinctrl-0 = <&pinctrl_gpio_keys &pinctrl_switch3_ixora>;
+
+		reset {
+			label = "reset";
+			gpios = <&gpio1 16 GPIO_ACTIVE_LOW>;
+			linux,code = <KEY_RESTART>;
+			debounce-interval = <10>;
+		};
+	};
+
 	reg_3v3_vmmc: regulator-3v3-vmmc {
 		compatible = "regulator-fixed";
 		enable-active-high;
@@ -264,6 +275,12 @@
 		>;
 	};
 
+	pinctrl_switch3_ixora: switch3ixora {
+		fsl,pins = <
+			MX6QDL_PAD_SD1_DAT0__GPIO1_IO16 0x1b0b0
+		>;
+	};
+
 	pinctrl_mmc_cd_sleep: mmccdslpgrp {
 		fsl,pins = <
 			 /* MMC1 CD */
