From 1861c63ba7bb7f8a5145d4ceabcf346f274da61f Mon Sep 17 00:00:00 2001
From: Frank Wunderlich <frank-w@public-files.de>
Date: Tue, 22 Apr 2025 15:24:30 +0200
Subject: [PATCH 28/32] arm64: dts: mediatek: mt7988: Add xsphy for
 ssusb0/pcie2

First usb and third pcie controller on mt7988 need a xs-phy to work
properly.

Signed-off-by: Frank Wunderlich <frank-w@public-files.de>
Reviewed-by: AngeloGioacchino Del Regno <angelogioacchino.delregno@collabora.com>
---
 arch/arm64/boot/dts/mediatek/mt7988a.dtsi | 36 +++++++++++++++++++++++
 1 file changed, 36 insertions(+)

--- a/arch/arm64/boot/dts/mediatek/mt7988a.dtsi
+++ b/arch/arm64/boot/dts/mediatek/mt7988a.dtsi
@@ -334,6 +334,8 @@
 				 <&infracfg CLK_INFRA_133M_USB_HCK>,
 				 <&infracfg CLK_INFRA_USB_XHCI>;
 			clock-names = "sys_ck", "ref_ck", "mcu_ck", "dma_ck", "xhci_ck";
+			phys = <&xphyu2port0 PHY_TYPE_USB2>,
+			       <&xphyu3port0 PHY_TYPE_USB3>;
 			status = "disabled";
 		};
 
@@ -398,6 +400,9 @@
 			pinctrl-0 = <&pcie2_pins>;
 			status = "disabled";
 
+			phys = <&xphyu3port0 PHY_TYPE_PCIE>;
+			phy-names = "pcie-phy";
+
 			#interrupt-cells = <1>;
 			interrupt-map-mask = <0 0 0 0x7>;
 			interrupt-map = <0 0 0 1 &pcie_intc2 0>,
@@ -548,6 +553,37 @@
 			};
 		};
 
+
+		topmisc: system-controller@11d10084 {
+			compatible = "mediatek,mt7988-topmisc",
+				     "syscon";
+			reg = <0 0x11d10084 0 0xff80>;
+		};
+
+		xs-phy@11e10000 {
+			compatible = "mediatek,mt7988-xsphy",
+				     "mediatek,xsphy";
+			#address-cells = <2>;
+			#size-cells = <2>;
+			ranges;
+			status = "disabled";
+
+			xphyu2port0: usb-phy@11e10000 {
+				reg = <0 0x11e10000 0 0x400>;
+				clocks = <&infracfg CLK_INFRA_USB_UTMI>;
+				clock-names = "ref";
+				#phy-cells = <1>;
+			};
+
+			xphyu3port0: usb-phy@11e13000 {
+				reg = <0 0x11e13400 0 0x500>;
+				clocks = <&infracfg CLK_INFRA_USB_PIPE>;
+				clock-names = "ref";
+				#phy-cells = <1>;
+				mediatek,syscon-type = <&topmisc 0x194 0>;
+			};
+		};
+
 		clock-controller@11f40000 {
 			compatible = "mediatek,mt7988-xfi-pll";
 			reg = <0 0x11f40000 0 0x1000>;
