From 05aba5763dcf35eddc58aaf99c9f16d19730e0a8 Mon Sep 17 00:00:00 2001
From: Cyrille Pitchen <cyrille.pitchen@atmel.com>
Date: Thu, 27 Oct 2016 11:55:39 +0200
Subject: [PATCH] mtd: spi-nor: rename SPINOR_OP_* macros of the 4-byte address
 op codes

This patch renames the SPINOR_OP_* macros of the 4-byte address
instruction set so the new names all share a common pattern: the 4-byte
address name is built from the 3-byte address name appending the "_4B"
suffix.

The patch also introduces new op codes to support other SPI protocols such
as SPI 1-4-4 and SPI 1-2-2.

This is a transitional patch and will help a later patch of spi-nor.c
to automate the translation from the 3-byte address op codes into their
4-byte address version.

Signed-off-by: Cyrille Pitchen <cyrille.pitchen@atmel.com>
Acked-by: Mark Brown <broonie@kernel.org>
Acked-by: Marek Vasut <marek.vasut@gmail.com>
---
 drivers/mtd/devices/serial_flash_cmds.h |  7 -------
 drivers/mtd/devices/st_spi_fsm.c        | 28 ++++++++++++++--------------
 drivers/mtd/spi-nor/spi-nor.c           |  8 ++++----
 drivers/spi/spi-bcm-qspi.c              |  6 +++---
 include/linux/mtd/spi-nor.h             | 22 ++++++++++++++++------
 5 files changed, 37 insertions(+), 34 deletions(-)

--- a/drivers/mtd/devices/serial_flash_cmds.h
+++ b/drivers/mtd/devices/serial_flash_cmds.h
@@ -18,19 +18,12 @@
 #define SPINOR_OP_RDVCR		0x85
 
 /* JEDEC Standard - Serial Flash Discoverable Parmeters (SFDP) Commands */
-#define SPINOR_OP_READ_1_2_2	0xbb	/* DUAL I/O READ */
-#define SPINOR_OP_READ_1_4_4	0xeb	/* QUAD I/O READ */
-
 #define SPINOR_OP_WRITE		0x02	/* PAGE PROGRAM */
 #define SPINOR_OP_WRITE_1_1_2	0xa2	/* DUAL INPUT PROGRAM */
 #define SPINOR_OP_WRITE_1_2_2	0xd2	/* DUAL INPUT EXT PROGRAM */
 #define SPINOR_OP_WRITE_1_1_4	0x32	/* QUAD INPUT PROGRAM */
 #define SPINOR_OP_WRITE_1_4_4	0x12	/* QUAD INPUT EXT PROGRAM */
 
-/* READ commands with 32-bit addressing */
-#define SPINOR_OP_READ4_1_2_2	0xbc
-#define SPINOR_OP_READ4_1_4_4	0xec
-
 /* Configuration flags */
 #define FLASH_FLAG_SINGLE	0x000000ff
 #define FLASH_FLAG_READ_WRITE	0x00000001
--- a/drivers/mtd/devices/st_spi_fsm.c
+++ b/drivers/mtd/devices/st_spi_fsm.c
@@ -507,13 +507,13 @@ static struct seq_rw_config n25q_read3_c
  *	- 'FAST' variants configured for 8 dummy cycles (see note above.)
  */
 static struct seq_rw_config n25q_read4_configs[] = {
-	{FLASH_FLAG_READ_1_4_4, SPINOR_OP_READ4_1_4_4,	0, 4, 4, 0x00, 0, 8},
-	{FLASH_FLAG_READ_1_1_4, SPINOR_OP_READ4_1_1_4,	0, 1, 4, 0x00, 0, 8},
-	{FLASH_FLAG_READ_1_2_2, SPINOR_OP_READ4_1_2_2,	0, 2, 2, 0x00, 0, 8},
-	{FLASH_FLAG_READ_1_1_2, SPINOR_OP_READ4_1_1_2,	0, 1, 2, 0x00, 0, 8},
-	{FLASH_FLAG_READ_FAST,	SPINOR_OP_READ4_FAST,	0, 1, 1, 0x00, 0, 8},
-	{FLASH_FLAG_READ_WRITE, SPINOR_OP_READ4,	0, 1, 1, 0x00, 0, 0},
-	{0x00,			0,			0, 0, 0, 0x00, 0, 0},
+	{FLASH_FLAG_READ_1_4_4, SPINOR_OP_READ_1_4_4_4B, 0, 4, 4, 0x00, 0, 8},
+	{FLASH_FLAG_READ_1_1_4, SPINOR_OP_READ_1_1_4_4B, 0, 1, 4, 0x00, 0, 8},
+	{FLASH_FLAG_READ_1_2_2, SPINOR_OP_READ_1_2_2_4B, 0, 2, 2, 0x00, 0, 8},
+	{FLASH_FLAG_READ_1_1_2, SPINOR_OP_READ_1_1_2_4B, 0, 1, 2, 0x00, 0, 8},
+	{FLASH_FLAG_READ_FAST,	SPINOR_OP_READ_FAST_4B,  0, 1, 1, 0x00, 0, 8},
+	{FLASH_FLAG_READ_WRITE, SPINOR_OP_READ_4B,       0, 1, 1, 0x00, 0, 0},
+	{0x00,			0,                       0, 0, 0, 0x00, 0, 0},
 };
 
 /*
@@ -553,13 +553,13 @@ static int stfsm_mx25_en_32bit_addr_seq(
  * entering a state that is incompatible with the SPIBoot Controller.
  */
 static struct seq_rw_config stfsm_s25fl_read4_configs[] = {
-	{FLASH_FLAG_READ_1_4_4,  SPINOR_OP_READ4_1_4_4,  0, 4, 4, 0x00, 2, 4},
-	{FLASH_FLAG_READ_1_1_4,  SPINOR_OP_READ4_1_1_4,  0, 1, 4, 0x00, 0, 8},
-	{FLASH_FLAG_READ_1_2_2,  SPINOR_OP_READ4_1_2_2,  0, 2, 2, 0x00, 4, 0},
-	{FLASH_FLAG_READ_1_1_2,  SPINOR_OP_READ4_1_1_2,  0, 1, 2, 0x00, 0, 8},
-	{FLASH_FLAG_READ_FAST,   SPINOR_OP_READ4_FAST,   0, 1, 1, 0x00, 0, 8},
-	{FLASH_FLAG_READ_WRITE,  SPINOR_OP_READ4,        0, 1, 1, 0x00, 0, 0},
-	{0x00,                   0,                      0, 0, 0, 0x00, 0, 0},
+	{FLASH_FLAG_READ_1_4_4,  SPINOR_OP_READ_1_4_4_4B,  0, 4, 4, 0x00, 2, 4},
+	{FLASH_FLAG_READ_1_1_4,  SPINOR_OP_READ_1_1_4_4B,  0, 1, 4, 0x00, 0, 8},
+	{FLASH_FLAG_READ_1_2_2,  SPINOR_OP_READ_1_2_2_4B,  0, 2, 2, 0x00, 4, 0},
+	{FLASH_FLAG_READ_1_1_2,  SPINOR_OP_READ_1_1_2_4B,  0, 1, 2, 0x00, 0, 8},
+	{FLASH_FLAG_READ_FAST,   SPINOR_OP_READ_FAST_4B,   0, 1, 1, 0x00, 0, 8},
+	{FLASH_FLAG_READ_WRITE,  SPINOR_OP_READ_4B,        0, 1, 1, 0x00, 0, 0},
+	{0x00,                   0,                        0, 0, 0, 0x00, 0, 0},
 };
 
 static struct seq_rw_config stfsm_s25fl_write4_configs[] = {
--- a/drivers/mtd/spi-nor/spi-nor.c
+++ b/drivers/mtd/spi-nor/spi-nor.c
@@ -1638,16 +1638,16 @@ int spi_nor_scan(struct spi_nor *nor, co
 			/* Dedicated 4-byte command set */
 			switch (nor->flash_read) {
 			case SPI_NOR_QUAD:
-				nor->read_opcode = SPINOR_OP_READ4_1_1_4;
+				nor->read_opcode = SPINOR_OP_READ_1_1_4_4B;
 				break;
 			case SPI_NOR_DUAL:
-				nor->read_opcode = SPINOR_OP_READ4_1_1_2;
+				nor->read_opcode = SPINOR_OP_READ_1_1_2_4B;
 				break;
 			case SPI_NOR_FAST:
-				nor->read_opcode = SPINOR_OP_READ4_FAST;
+				nor->read_opcode = SPINOR_OP_READ_FAST_4B;
 				break;
 			case SPI_NOR_NORMAL:
-				nor->read_opcode = SPINOR_OP_READ4;
+				nor->read_opcode = SPINOR_OP_READ_4B;
 				break;
 			}
 			nor->program_opcode = SPINOR_OP_PP_4B;
--- a/drivers/spi/spi-bcm-qspi.c
+++ b/drivers/spi/spi-bcm-qspi.c
@@ -371,7 +371,7 @@ static int bcm_qspi_bspi_set_flex_mode(s
 			/* default mode, does not need flex_cmd */
 			flex_mode = 0;
 		else
-			command = SPINOR_OP_READ4_FAST;
+			command = SPINOR_OP_READ_FAST_4B;
 		break;
 	case SPI_NBITS_DUAL:
 		bpc = 0x00000001;
@@ -384,7 +384,7 @@ static int bcm_qspi_bspi_set_flex_mode(s
 		} else {
 			command = SPINOR_OP_READ_1_1_2;
 			if (spans_4byte)
-				command = SPINOR_OP_READ4_1_1_2;
+				command = SPINOR_OP_READ_1_1_2_4B;
 		}
 		break;
 	case SPI_NBITS_QUAD:
@@ -399,7 +399,7 @@ static int bcm_qspi_bspi_set_flex_mode(s
 		} else {
 			command = SPINOR_OP_READ_1_1_4;
 			if (spans_4byte)
-				command = SPINOR_OP_READ4_1_1_4;
+				command = SPINOR_OP_READ_1_1_4_4B;
 		}
 		break;
 	default:
--- a/include/linux/mtd/spi-nor.h
+++ b/include/linux/mtd/spi-nor.h
@@ -43,9 +43,13 @@
 #define SPINOR_OP_WRSR		0x01	/* Write status register 1 byte */
 #define SPINOR_OP_READ		0x03	/* Read data bytes (low frequency) */
 #define SPINOR_OP_READ_FAST	0x0b	/* Read data bytes (high frequency) */
-#define SPINOR_OP_READ_1_1_2	0x3b	/* Read data bytes (Dual SPI) */
-#define SPINOR_OP_READ_1_1_4	0x6b	/* Read data bytes (Quad SPI) */
+#define SPINOR_OP_READ_1_1_2	0x3b	/* Read data bytes (Dual Output SPI) */
+#define SPINOR_OP_READ_1_2_2	0xbb	/* Read data bytes (Dual I/O SPI) */
+#define SPINOR_OP_READ_1_1_4	0x6b	/* Read data bytes (Quad Output SPI) */
+#define SPINOR_OP_READ_1_4_4	0xeb	/* Read data bytes (Quad I/O SPI) */
 #define SPINOR_OP_PP		0x02	/* Page program (up to 256 bytes) */
+#define SPINOR_OP_PP_1_1_4	0x32	/* Quad page program */
+#define SPINOR_OP_PP_1_4_4	0x38	/* Quad page program */
 #define SPINOR_OP_BE_4K		0x20	/* Erase 4KiB block */
 #define SPINOR_OP_BE_4K_PMC	0xd7	/* Erase 4KiB block on PMC chips */
 #define SPINOR_OP_BE_32K	0x52	/* Erase 32KiB block */
@@ -56,11 +60,17 @@
 #define SPINOR_OP_RDFSR		0x70	/* Read flag status register */
 
 /* 4-byte address opcodes - used on Spansion and some Macronix flashes. */
-#define SPINOR_OP_READ4		0x13	/* Read data bytes (low frequency) */
-#define SPINOR_OP_READ4_FAST	0x0c	/* Read data bytes (high frequency) */
-#define SPINOR_OP_READ4_1_1_2	0x3c	/* Read data bytes (Dual SPI) */
-#define SPINOR_OP_READ4_1_1_4	0x6c	/* Read data bytes (Quad SPI) */
+#define SPINOR_OP_READ_4B	0x13	/* Read data bytes (low frequency) */
+#define SPINOR_OP_READ_FAST_4B	0x0c	/* Read data bytes (high frequency) */
+#define SPINOR_OP_READ_1_1_2_4B	0x3c	/* Read data bytes (Dual Output SPI) */
+#define SPINOR_OP_READ_1_2_2_4B	0xbc	/* Read data bytes (Dual I/O SPI) */
+#define SPINOR_OP_READ_1_1_4_4B	0x6c	/* Read data bytes (Quad Output SPI) */
+#define SPINOR_OP_READ_1_4_4_4B	0xec	/* Read data bytes (Quad I/O SPI) */
 #define SPINOR_OP_PP_4B		0x12	/* Page program (up to 256 bytes) */
+#define SPINOR_OP_PP_1_1_4_4B	0x34	/* Quad page program */
+#define SPINOR_OP_PP_1_4_4_4B	0x3e	/* Quad page program */
+#define SPINOR_OP_BE_4K_4B	0x21	/* Erase 4KiB block */
+#define SPINOR_OP_BE_32K_4B	0x5c	/* Erase 32KiB block */
 #define SPINOR_OP_SE_4B		0xdc	/* Sector erase (usually 64KiB) */
 
 /* Used for SST flashes only. */
