/dts-v1/;

#include "mt7621.dtsi"

#include <dt-bindings/input/input.h>
#include <dt-bindings/gpio/gpio.h>

/ {
	compatible = "mikrotik,rbm33g", "mediatek,mt7621-soc";
	model = "MikroTik RBM33G";

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x10000000>;
	};

	chosen {
		bootargs = "console=ttyS0,115200";
	};

	gpio-leds {
		compatible = "gpio-leds";

		usr {
			label = "rbm33g:green:usr";
			gpios = <&gpio0 0 GPIO_ACTIVE_HIGH>;
		};

	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <20>;

		res {
			label = "res";
			gpios = <&gpio0 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	pcie0_vcc_reg {
		compatible = "regulator-fixed";
		regulator-name = "pcie0_vcc";

		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		gpio = <&gpio0 9 GPIO_ACTIVE_HIGH>;
		enable-active-high;
		regulator-boot-on;
		regulator-always-on;
	};

	pcie1_vcc_reg {
		compatible = "regulator-fixed";
		regulator-name = "pcie1_vcc";

		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		gpio = <&gpio0 10 GPIO_ACTIVE_HIGH>;
		enable-active-high;
		regulator-boot-on;
		regulator-always-on;
	};

	pcie2_vcc_reg {
		compatible = "regulator-fixed";
		regulator-name = "pcie2_vcc";

		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		gpio = <&gpio0 11 GPIO_ACTIVE_HIGH>;
		enable-active-high;
		regulator-boot-on;
		regulator-always-on;
	};

	usb_vcc_reg {
		compatible = "regulator-fixed";
		regulator-name = "usb_vcc";

		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		gpio = <&gpio0 12 GPIO_ACTIVE_HIGH>;
		enable-active-high;
		regulator-always-on;
	};
};


&spi0 {
	status = "okay";

	w25q40@0 {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <3125000>;

		partition@0 {
			label = "routerboot";
			reg = <0x0 0xf000>;
			read-only;
		};

		factory: partition@f000 {
			label = "factory";
			reg = <0xf000 0x71000>;
			read-only;
		};

	};

	w25q128@0 {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "jedec,spi-nor";
		reg = <1>;
		spi-max-frequency = <3125000>;

		partition@40000 {
			label = "firmware";
			reg = <0x040000 0xFC0000>;
		};
	};
};

&ethernet {
	mtd-mac-address = <&factory 0x0010>;
	mtd-mac-address-increment = <1>;
};


&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "uart2", "wdt";
			ralink,function = "gpio";
		};
	};
};

&sdhci {
	status = "okay";
};

&i2c {
	status = "okay";
};

&pcie {
	status = "okay";
};
