From: Lorenzo Bianconi <lorenzo.bianconi@redhat.com>
Date: Fri, 2 Nov 2018 21:49:56 +0100
Subject: [PATCH] ath9k: dynack: move debug log after buffer increments

Move debug log in ath_dynack_sample_tx_ts and ath_dynack_sample_ack_ts
after timestamp buffer head/tail increments in order to make debugging
more user friendly

Tested-by: Koen Vandeputte <koen.vandeputte@ncentric.com>
Signed-off-by: Lorenzo Bianconi <lorenzo.bianconi@redhat.com>
---

--- a/drivers/net/wireless/ath/ath9k/dynack.c
+++ b/drivers/net/wireless/ath/ath9k/dynack.c
@@ -171,11 +171,12 @@ static void ath_dynack_compute_to(struct
 void ath_dynack_sample_tx_ts(struct ath_hw *ah, struct sk_buff *skb,
 			     struct ath_tx_status *ts)
 {
-	u8 ridx;
 	struct ieee80211_hdr *hdr;
 	struct ath_dynack *da = &ah->dynack;
 	struct ath_common *common = ath9k_hw_common(ah);
 	struct ieee80211_tx_info *info = IEEE80211_SKB_CB(skb);
+	u32 dur = ts->duration;
+	u8 ridx;
 
 	if ((info->flags & IEEE80211_TX_CTL_NO_ACK) || !da->enabled)
 		return;
@@ -203,14 +204,13 @@ void ath_dynack_sample_tx_ts(struct ath_
 	ridx = ts->ts_rateindex;
 
 	da->st_rbf.ts[da->st_rbf.t_rb].tstamp = ts->ts_tstamp;
-	da->st_rbf.ts[da->st_rbf.t_rb].dur = ts->duration;
 	ether_addr_copy(da->st_rbf.addr[da->st_rbf.t_rb].h_dest, hdr->addr1);
 	ether_addr_copy(da->st_rbf.addr[da->st_rbf.t_rb].h_src, hdr->addr2);
 
 	if (!(info->status.rates[ridx].flags & IEEE80211_TX_RC_MCS)) {
-		u32 phy, sifs;
 		const struct ieee80211_rate *rate;
 		struct ieee80211_tx_rate *rates = info->status.rates;
+		u32 phy;
 
 		rate = &common->sbands[info->band].bitrates[rates[ridx].idx];
 		if (info->band == NL80211_BAND_2GHZ &&
@@ -219,19 +219,18 @@ void ath_dynack_sample_tx_ts(struct ath_
 		else
 			phy = WLAN_RC_PHY_OFDM;
 
-		sifs = ath_dynack_get_sifs(ah, phy);
-		da->st_rbf.ts[da->st_rbf.t_rb].dur -= sifs;
+		dur -= ath_dynack_get_sifs(ah, phy);
 	}
-
-	ath_dbg(common, DYNACK, "{%pM} tx sample %u [dur %u][h %u-t %u]\n",
-		hdr->addr1, da->st_rbf.ts[da->st_rbf.t_rb].tstamp,
-		da->st_rbf.ts[da->st_rbf.t_rb].dur, da->st_rbf.h_rb,
-		(da->st_rbf.t_rb + 1) % ATH_DYN_BUF);
+	da->st_rbf.ts[da->st_rbf.t_rb].dur = dur;
 
 	INCR(da->st_rbf.t_rb, ATH_DYN_BUF);
 	if (da->st_rbf.t_rb == da->st_rbf.h_rb)
 		INCR(da->st_rbf.h_rb, ATH_DYN_BUF);
 
+	ath_dbg(common, DYNACK, "{%pM} tx sample %u [dur %u][h %u-t %u]\n",
+		hdr->addr1, ts->ts_tstamp, dur, da->st_rbf.h_rb,
+		da->st_rbf.t_rb);
+
 	ath_dynack_compute_to(ah);
 
 	spin_unlock_bh(&da->qlock);
@@ -258,14 +257,13 @@ void ath_dynack_sample_ack_ts(struct ath
 	spin_lock_bh(&da->qlock);
 	da->ack_rbf.tstamp[da->ack_rbf.t_rb] = ts;
 
-	ath_dbg(common, DYNACK, "rx sample %u [h %u-t %u]\n",
-		da->ack_rbf.tstamp[da->ack_rbf.t_rb],
-		da->ack_rbf.h_rb, (da->ack_rbf.t_rb + 1) % ATH_DYN_BUF);
-
 	INCR(da->ack_rbf.t_rb, ATH_DYN_BUF);
 	if (da->ack_rbf.t_rb == da->ack_rbf.h_rb)
 		INCR(da->ack_rbf.h_rb, ATH_DYN_BUF);
 
+	ath_dbg(common, DYNACK, "rx sample %u [h %u-t %u]\n",
+		ts, da->ack_rbf.h_rb, da->ack_rbf.t_rb);
+
 	ath_dynack_compute_to(ah);
 
 	spin_unlock_bh(&da->qlock);
