From a9d2b105ccd23e07e3dd99d010a34bd5d1c95b42 Mon Sep 17 00:00:00 2001
From: Daniel Golle <daniel@makrotopia.org>
Date: Sat, 13 Jan 2018 18:35:59 +0100
Subject: [PATCH 1/3] ARM: dts: rename oxnas dts files

Other platforms' device-tree files start with a platform prefix, such as
sun7i-a20-*.dts or at91-*.dts.
This naming scheme turns out to be handy when using multi-platform build
systems such as OpenWrt.
Prepend oxnas files with their platform prefix to comply with the naming
scheme already used for most other platforms.

Signed-off-by: Daniel Golle <daniel@makrotopia.org>
Signed-off-by: Arnd Bergmann <arnd@arndb.de>
---
 arch/arm/boot/dts/Makefile                                    | 4 ++--
 arch/arm/boot/dts/{wd-mbwe.dts => ox810se-wd-mbwe.dts}        | 0
 ...-series-3.dts => ox820-cloudengines-pogoplug-series-3.dts} | 0
 3 files changed, 2 insertions(+), 2 deletions(-)
 rename arch/arm/boot/dts/{wd-mbwe.dts => ox810se-wd-mbwe.dts} (100%)
 rename arch/arm/boot/dts/{cloudengines-pogoplug-series-3.dts => ox820-cloudengines-pogoplug-series-3.dts} (100%)

--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -685,8 +685,8 @@ dtb-$(CONFIG_ARCH_ACTIONS) += \
 dtb-$(CONFIG_ARCH_PRIMA2) += \
 	prima2-evb.dtb
 dtb-$(CONFIG_ARCH_OXNAS) += \
-	wd-mbwe.dtb \
-	cloudengines-pogoplug-series-3.dtb
+	ox810se-wd-mbwe.dtb \
+	ox820-cloudengines-pogoplug-series-3.dtb
 dtb-$(CONFIG_ARCH_QCOM) += \
 	qcom-apq8060-dragonboard.dtb \
 	qcom-apq8064-arrow-sd-600eval.dtb \
--- a/arch/arm/boot/dts/cloudengines-pogoplug-series-3.dts
+++ /dev/null
@@ -1,94 +0,0 @@
-/*
- * cloudengines-pogoplug-series-3.dtsi - Device tree file for Cloud Engines PogoPlug Series 3
- *
- * Copyright (C) 2016 Neil Armstrong <narmstrong@baylibre.com>
- *
- * Licensed under GPLv2 or later
- */
-
-/dts-v1/;
-#include "ox820.dtsi"
-
-/ {
-	model = "Cloud Engines PogoPlug Series 3";
-
-	compatible = "cloudengines,pogoplugv3", "oxsemi,ox820";
-
-	chosen {
-		bootargs = "earlyprintk";
-		stdout-path = "serial0:115200n8";
-	};
-
-	memory {
-		/* 128Mbytes DDR */
-		reg = <0x60000000 0x8000000>;
-	};
-
-	aliases {
-		serial0 = &uart0;
-		gpio0 = &gpio0;
-		gpio1 = &gpio1;
-	};
-
-	leds {
-		compatible = "gpio-leds";
-
-		blue {
-			label = "pogoplug:blue";
-			gpios = <&gpio0 2 0>;
-			default-state = "keep";
-		};
-
-		orange {
-			label = "pogoplug:orange";
-			gpios = <&gpio1 16 1>;
-			default-state = "keep";
-		};
-
-		green {
-			label = "pogoplug:green";
-			gpios = <&gpio1 17 1>;
-			default-state = "keep";
-		};
-	};
-};
-
-&uart0 {
-	status = "okay";
-
-	pinctrl-names = "default";
-	pinctrl-0 = <&pinctrl_uart0>;
-};
-
-&nandc {
-	status = "okay";
-
-	pinctrl-names = "default";
-	pinctrl-0 = <&pinctrl_nand>;
-
-	nand@0 {
-		reg = <0>;
-		#address-cells = <1>;
-		#size-cells = <1>;
-		nand-ecc-mode = "soft";
-		nand-ecc-algo = "hamming";
-
-		partition@0 {
-			label = "boot";
-			reg = <0x00000000 0x00e00000>;
-			read-only;
-		};
-
-		partition@e00000 {
-			label = "ubi";
-			reg = <0x00e00000 0x07200000>;
-		};
-	};
-};
-
-&etha {
-	status = "okay";
-
-	pinctrl-names = "default";
-	pinctrl-0 = <&pinctrl_etha_mdio>;
-};
--- /dev/null
+++ b/arch/arm/boot/dts/ox810se-wd-mbwe.dts
@@ -0,0 +1,112 @@
+/*
+ * wd-mbwe.dtsi - Device tree file for Western Digital My Book World Edition
+ *
+ * Copyright (C) 2016 Neil Armstrong <narmstrong@baylibre.com>
+ *
+ * Licensed under GPLv2 or later
+ */
+
+/dts-v1/;
+#include "ox810se.dtsi"
+
+/ {
+	model = "Western Digital My Book World Edition";
+
+	compatible = "wd,mbwe", "oxsemi,ox810se";
+
+	chosen {
+		bootargs = "console=ttyS1,115200n8 earlyprintk=serial";
+	};
+
+	memory {
+		/* 128Mbytes DDR */
+		reg = <0x48000000 0x8000000>;
+	};
+
+	aliases {
+		serial1 = &uart1;
+		gpio0 = &gpio0;
+		gpio1 = &gpio1;
+	};
+
+	gpio-keys-polled {
+		compatible = "gpio-keys-polled";
+		#address-cells = <1>;
+		#size-cells = <0>;
+		poll-interval = <100>;
+
+		power {
+			label = "power";
+			gpios = <&gpio0 0 1>;
+			linux,code = <0x198>;
+		};
+
+		recovery {
+			label = "recovery";
+			gpios = <&gpio0 4 1>;
+			linux,code = <0xab>;
+		};
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		a0 {
+			label = "activity0";
+			gpios = <&gpio0 25 0>;
+			default-state = "keep";
+		};
+
+		a1 {
+			label = "activity1";
+			gpios = <&gpio0 26 0>;
+			default-state = "keep";
+		};
+
+		a2 {
+			label = "activity2";
+			gpios = <&gpio0 5 0>;
+			default-state = "keep";
+		};
+
+		a3 {
+			label = "activity3";
+			gpios = <&gpio0 6 0>;
+			default-state = "keep";
+		};
+
+		a4 {
+			label = "activity4";
+			gpios = <&gpio0 7 0>;
+			default-state = "keep";
+		};
+
+		a5 {
+			label = "activity5";
+			gpios = <&gpio1 2 0>;
+			default-state = "keep";
+		};
+	};
+
+	i2c-gpio {
+		compatible = "i2c-gpio";
+		gpios = <&gpio0 3 0 /* sda */
+			 &gpio0 2 0 /* scl */
+			 >;
+		i2c-gpio,delay-us = <2>;        /* ~100 kHz */
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		rtc0: rtc@48 {
+			compatible = "st,m41t00";
+			reg = <0x68>;
+		};
+	};
+};
+
+&uart1 {
+	status = "okay";
+
+	pinctrl-names = "default";
+	pinctrl-0 = <&pinctrl_uart1>;
+};
--- /dev/null
+++ b/arch/arm/boot/dts/ox820-cloudengines-pogoplug-series-3.dts
@@ -0,0 +1,94 @@
+/*
+ * cloudengines-pogoplug-series-3.dtsi - Device tree file for Cloud Engines PogoPlug Series 3
+ *
+ * Copyright (C) 2016 Neil Armstrong <narmstrong@baylibre.com>
+ *
+ * Licensed under GPLv2 or later
+ */
+
+/dts-v1/;
+#include "ox820.dtsi"
+
+/ {
+	model = "Cloud Engines PogoPlug Series 3";
+
+	compatible = "cloudengines,pogoplugv3", "oxsemi,ox820";
+
+	chosen {
+		bootargs = "earlyprintk";
+		stdout-path = "serial0:115200n8";
+	};
+
+	memory {
+		/* 128Mbytes DDR */
+		reg = <0x60000000 0x8000000>;
+	};
+
+	aliases {
+		serial0 = &uart0;
+		gpio0 = &gpio0;
+		gpio1 = &gpio1;
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		blue {
+			label = "pogoplug:blue";
+			gpios = <&gpio0 2 0>;
+			default-state = "keep";
+		};
+
+		orange {
+			label = "pogoplug:orange";
+			gpios = <&gpio1 16 1>;
+			default-state = "keep";
+		};
+
+		green {
+			label = "pogoplug:green";
+			gpios = <&gpio1 17 1>;
+			default-state = "keep";
+		};
+	};
+};
+
+&uart0 {
+	status = "okay";
+
+	pinctrl-names = "default";
+	pinctrl-0 = <&pinctrl_uart0>;
+};
+
+&nandc {
+	status = "okay";
+
+	pinctrl-names = "default";
+	pinctrl-0 = <&pinctrl_nand>;
+
+	nand@0 {
+		reg = <0>;
+		#address-cells = <1>;
+		#size-cells = <1>;
+		nand-ecc-mode = "soft";
+		nand-ecc-algo = "hamming";
+
+		partition@0 {
+			label = "boot";
+			reg = <0x00000000 0x00e00000>;
+			read-only;
+		};
+
+		partition@e00000 {
+			label = "ubi";
+			reg = <0x00e00000 0x07200000>;
+		};
+	};
+};
+
+&etha {
+	status = "okay";
+
+	pinctrl-names = "default";
+	pinctrl-0 = <&pinctrl_etha_mdio>;
+};
--- a/arch/arm/boot/dts/wd-mbwe.dts
+++ /dev/null
@@ -1,112 +0,0 @@
-/*
- * wd-mbwe.dtsi - Device tree file for Western Digital My Book World Edition
- *
- * Copyright (C) 2016 Neil Armstrong <narmstrong@baylibre.com>
- *
- * Licensed under GPLv2 or later
- */
-
-/dts-v1/;
-#include "ox810se.dtsi"
-
-/ {
-	model = "Western Digital My Book World Edition";
-
-	compatible = "wd,mbwe", "oxsemi,ox810se";
-
-	chosen {
-		bootargs = "console=ttyS1,115200n8 earlyprintk=serial";
-	};
-
-	memory {
-		/* 128Mbytes DDR */
-		reg = <0x48000000 0x8000000>;
-	};
-
-	aliases {
-		serial1 = &uart1;
-		gpio0 = &gpio0;
-		gpio1 = &gpio1;
-	};
-
-	gpio-keys-polled {
-		compatible = "gpio-keys-polled";
-		#address-cells = <1>;
-		#size-cells = <0>;
-		poll-interval = <100>;
-
-		power {
-			label = "power";
-			gpios = <&gpio0 0 1>;
-			linux,code = <0x198>;
-		};
-
-		recovery {
-			label = "recovery";
-			gpios = <&gpio0 4 1>;
-			linux,code = <0xab>;
-		};
-	};
-
-	leds {
-		compatible = "gpio-leds";
-
-		a0 {
-			label = "activity0";
-			gpios = <&gpio0 25 0>;
-			default-state = "keep";
-		};
-
-		a1 {
-			label = "activity1";
-			gpios = <&gpio0 26 0>;
-			default-state = "keep";
-		};
-
-		a2 {
-			label = "activity2";
-			gpios = <&gpio0 5 0>;
-			default-state = "keep";
-		};
-
-		a3 {
-			label = "activity3";
-			gpios = <&gpio0 6 0>;
-			default-state = "keep";
-		};
-
-		a4 {
-			label = "activity4";
-			gpios = <&gpio0 7 0>;
-			default-state = "keep";
-		};
-
-		a5 {
-			label = "activity5";
-			gpios = <&gpio1 2 0>;
-			default-state = "keep";
-		};
-	};
-
-	i2c-gpio {
-		compatible = "i2c-gpio";
-		gpios = <&gpio0 3 0 /* sda */
-			 &gpio0 2 0 /* scl */
-			 >;
-		i2c-gpio,delay-us = <2>;        /* ~100 kHz */
-		#address-cells = <1>;
-		#size-cells = <0>;
-
-		rtc0: rtc@48 {
-			compatible = "st,m41t00";
-			reg = <0x68>;
-		};
-	};
-};
-
-&uart1 {
-	status = "okay";
-
-	pinctrl-names = "default";
-	pinctrl-0 = <&pinctrl_uart1>;
-};
