From: Felix Fietkau <nbd@nbd.name>
Date: Sat, 29 Sep 2018 15:55:44 +0200
Subject: [PATCH] mac80211: fix setting IEEE80211_KEY_FLAG_RX_MGMT for AP mode
 keys

key->sta is only valid after ieee80211_key_link, which is called later
in this function. Because of that, the IEEE80211_KEY_FLAG_RX_MGMT is
never set when management frame protection is enabled.

Fixes: e548c49e6dc6b ("mac80211: add key flag for management keys")
Cc: stable@vger.kernel.org
Signed-off-by: Felix Fietkau <nbd@nbd.name>
---

--- a/net/mac80211/cfg.c
+++ b/net/mac80211/cfg.c
@@ -426,7 +426,7 @@ static int ieee80211_add_key(struct wiph
 	case NL80211_IFTYPE_AP:
 	case NL80211_IFTYPE_AP_VLAN:
 		/* Keys without a station are used for TX only */
-		if (key->sta && test_sta_flag(key->sta, WLAN_STA_MFP))
+		if (sta && test_sta_flag(sta, WLAN_STA_MFP))
 			key->conf.flags |= IEEE80211_KEY_FLAG_RX_MGMT;
 		break;
 	case NL80211_IFTYPE_ADHOC:
