--- a/drivers/net/wireless/broadcom/b43/main.c
+++ b/drivers/net/wireless/broadcom/b43/main.c
@@ -2909,6 +2909,14 @@ static int b43_gpio_init(struct b43_wlde
 	} else if (dev->dev->chip_id == 0x5354) {
 		/* Don't allow overtaking buttons GPIOs */
 		set &= 0x2; /* 0x2 is LED GPIO on BCM5354 */
+	} else if (dev->dev->chip_id == BCMA_CHIP_ID_BCM4716 || 
+		   dev->dev->chip_id == BCMA_CHIP_ID_BCM47162 ||
+		   dev->dev->chip_id == BCMA_CHIP_ID_BCM5356 ||
+		   dev->dev->chip_id == BCMA_CHIP_ID_BCM5357 ||
+		   dev->dev->chip_id == BCMA_CHIP_ID_BCM53572) {
+		/* just use gpio 0 and 1 for 2.4 GHz wifi led */
+		set &= 0x3;
+		mask &= 0x3;
 	}
 
 	if (0 /* FIXME: conditional unknown */ ) {
