From 2fef681a4cf7994c882190fd2417b95f30510afb Mon Sep 17 00:00:00 2001
From: Jia-Shyr Chuang <saint.chuang@cypress.com>
Date: Wed, 15 Aug 2018 04:23:09 -0500
Subject: [PATCH] brcmfmac: add CYW89342 mini-PCIe device

CYW89342 is a 2x2 MIMO, 802.11a/b/g/n/ac for WLAN. It is a member of
4355/4359 family.

Signed-off-by: Jia-Shyr Chuang <saint.chuang@cypress.com>
Signed-off-by: Chi-Hsien Lin <chi-hsien.lin@cypress.com>
Signed-off-by: Kalle Valo <kvalo@codeaurora.org>
---
 drivers/net/wireless/broadcom/brcm80211/brcmfmac/pcie.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/pcie.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/pcie.c
@@ -2017,6 +2017,7 @@ static const struct dev_pm_ops brcmf_pci
 
 static const struct pci_device_id brcmf_pcie_devid_table[] = {
 	BRCMF_PCIE_DEVICE(BRCM_PCIE_4350_DEVICE_ID),
+	BRCMF_PCIE_DEVICE_SUB(0x4355, BRCM_PCIE_VENDOR_ID_BROADCOM, 0x4355),
 	BRCMF_PCIE_DEVICE(BRCM_PCIE_4356_DEVICE_ID),
 	BRCMF_PCIE_DEVICE(BRCM_PCIE_43567_DEVICE_ID),
 	BRCMF_PCIE_DEVICE(BRCM_PCIE_43570_DEVICE_ID),
