From 5a4326d3a03f03c2518a2c255be33a7114af3230 Mon Sep 17 00:00:00 2001
From: Christian Lamparter <chunkeey@gmail.com>
Date: Wed, 4 Oct 2017 01:00:05 +0200
Subject: [PATCH 13/25] crypto: crypto4xx - wire up hmac_mc to hmac_muting

The hmac_mc parameter of set_dynamic_sa_command_1()
was defined but not used. On closer inspection it
turns out, it was never wired up.

Signed-off-by: Christian Lamparter <chunkeey@gmail.com>
Signed-off-by: Herbert Xu <herbert@gondor.apana.org.au>
---
 drivers/crypto/amcc/crypto4xx_alg.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/crypto/amcc/crypto4xx_alg.c
+++ b/drivers/crypto/amcc/crypto4xx_alg.c
@@ -63,6 +63,7 @@ static void set_dynamic_sa_command_1(str
 	sa->sa_command_1.bf.crypto_mode9_8 = cm & 3;
 	sa->sa_command_1.bf.feedback_mode = cfb,
 	sa->sa_command_1.bf.sa_rev = 1;
+	sa->sa_command_1.bf.hmac_muting = hmac_mc;
 	sa->sa_command_1.bf.extended_seq_num = esn;
 	sa->sa_command_1.bf.seq_num_mask = sn_mask;
 	sa->sa_command_1.bf.mutable_bit_proc = mute;
