--- a/arch/arm/boot/dts/qcom-ipq4019-ap.dk01.1.dtsi
+++ b/arch/arm/boot/dts/qcom-ipq4019-ap.dk01.1.dtsi
@@ -15,12 +15,39 @@
  */
 
 #include "qcom-ipq4019.dtsi"
+#include <dt-bindings/soc/qcom,tcsr.h>
 
 / {
 	model = "Qualcomm Technologies, Inc. IPQ4019/AP-DK01.1";
 	compatible = "qcom,ipq4019";
 
 	soc {
+		tcsr@194b000 {
+			/* select hostmode */
+			compatible = "qcom,tcsr";
+			reg = <0x194b000 0x100>;
+			qcom,usb-hsphy-mode-select = <TCSR_USB_HSPHY_HOST_MODE>;
+			status = "ok";
+		};
+
+		ess_tcsr@1953000 {
+			compatible = "qcom,tcsr";
+			reg = <0x1953000 0x1000>;
+			qcom,ess-interface-select = <TCSR_ESS_PSGMII>;
+		};
+
+		tcsr@1949000 {
+			compatible = "qcom,tcsr";
+			reg = <0x1949000 0x100>;
+			qcom,wifi_glb_cfg = <TCSR_WIFI_GLB_CFG>;
+		};
+
+		tcsr@1957000 {
+			compatible = "qcom,tcsr";
+			reg = <0x1957000 0x100>;
+			qcom,wifi_noc_memtype_m0_m2 = <TCSR_WIFI_NOC_MEMTYPE_M0_M2>;
+		};
+
 		rng@22000 {
 			status = "ok";
 		};
