From 6710c5b0674f8811f7d8fbfc526684e7ed77f765 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Thu, 11 Feb 2021 13:12:32 +0100
Subject: [PATCH] dt-bindings: net: rename BCM4908 Ethernet binding
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Rob pointed out that a normal convention is "brcm,bcm4908-enet" so
update whole binding to match it.

Suggested-by: Rob Herring <robh@kernel.org>
Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
Reviewed-by: Florian Fainelli <f.fainelli@gmail.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 .../net/{brcm,bcm4908enet.yaml => brcm,bcm4908-enet.yaml}   | 6 +++---
 MAINTAINERS                                                 | 2 +-
 2 files changed, 4 insertions(+), 4 deletions(-)
 rename Documentation/devicetree/bindings/net/{brcm,bcm4908enet.yaml => brcm,bcm4908-enet.yaml} (85%)

--- a/Documentation/devicetree/bindings/net/brcm,bcm4908enet.yaml
+++ /dev/null
@@ -1,45 +0,0 @@
-# SPDX-License-Identifier: GPL-2.0-only OR BSD-2-Clause
-%YAML 1.2
----
-$id: http://devicetree.org/schemas/net/brcm,bcm4908enet.yaml#
-$schema: http://devicetree.org/meta-schemas/core.yaml#
-
-title: Broadcom BCM4908 Ethernet controller
-
-description: Broadcom's Ethernet controller integrated into BCM4908 family SoCs
-
-maintainers:
-  - Rafał Miłecki <rafal@milecki.pl>
-
-properties:
-  compatible:
-    const: brcm,bcm4908enet
-
-  reg:
-    maxItems: 1
-
-  interrupts:
-    description: RX interrupt
-
-  interrupt-names:
-    const: rx
-
-required:
-  - reg
-  - interrupts
-  - interrupt-names
-
-additionalProperties: false
-
-examples:
-  - |
-    #include <dt-bindings/interrupt-controller/irq.h>
-    #include <dt-bindings/interrupt-controller/arm-gic.h>
-
-    ethernet@80002000 {
-        compatible = "brcm,bcm4908enet";
-        reg = <0x80002000 0x1000>;
-
-        interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>;
-        interrupt-names = "rx";
-    };
--- /dev/null
+++ b/Documentation/devicetree/bindings/net/brcm,bcm4908-enet.yaml
@@ -0,0 +1,45 @@
+# SPDX-License-Identifier: GPL-2.0-only OR BSD-2-Clause
+%YAML 1.2
+---
+$id: http://devicetree.org/schemas/net/brcm,bcm4908-enet.yaml#
+$schema: http://devicetree.org/meta-schemas/core.yaml#
+
+title: Broadcom BCM4908 Ethernet controller
+
+description: Broadcom's Ethernet controller integrated into BCM4908 family SoCs
+
+maintainers:
+  - Rafał Miłecki <rafal@milecki.pl>
+
+properties:
+  compatible:
+    const: brcm,bcm4908-enet
+
+  reg:
+    maxItems: 1
+
+  interrupts:
+    description: RX interrupt
+
+  interrupt-names:
+    const: rx
+
+required:
+  - reg
+  - interrupts
+  - interrupt-names
+
+additionalProperties: false
+
+examples:
+  - |
+    #include <dt-bindings/interrupt-controller/irq.h>
+    #include <dt-bindings/interrupt-controller/arm-gic.h>
+
+    ethernet@80002000 {
+        compatible = "brcm,bcm4908-enet";
+        reg = <0x80002000 0x1000>;
+
+        interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>;
+        interrupt-names = "rx";
+    };
--- a/MAINTAINERS
+++ b/MAINTAINERS
@@ -3432,7 +3432,7 @@ M:	Rafał Miłecki <rafal@milecki.pl>
 M:	bcm-kernel-feedback-list@broadcom.com
 L:	netdev@vger.kernel.org
 S:	Maintained
-F:	Documentation/devicetree/bindings/net/brcm,bcm4908enet.yaml
+F:	Documentation/devicetree/bindings/net/brcm,bcm4908-enet.yaml
 F:	drivers/net/ethernet/broadcom/bcm4908enet.*
 F:	drivers/net/ethernet/broadcom/unimac.h
 
