From 0dd369ae91c3c4d2db2aa292935d12db5a0d97e1 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime@cerno.tech>
Date: Wed, 28 Oct 2020 13:32:22 +0100
Subject: [PATCH] drm/atomic: Pass the full state to CRTC atomic begin
 and flush
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Commit f6ebe9f9c9233a6114eb922aba9a0c9ccc2d2e14 upstream.

The current atomic helpers have either their object state being passed as
an argument or the full atomic state.

The former is the pattern that was done at first, before switching to the
latter for new hooks or when it was needed.

Let's start convert all the remaining helpers to provide a consistent
interface, starting with the CRTC's atomic_begin and atomic_flush.

The conversion was done using the coccinelle script below, built tested on
all the drivers and actually tested on vc4.

virtual report

@@
struct drm_crtc_helper_funcs *FUNCS;
identifier old_crtc_state, old_state;
identifier crtc;
identifier f;
@@

 f(struct drm_crtc_state *old_crtc_state)
 {
	...
 	struct drm_atomic_state *old_state = old_crtc_state->state;
	<...
-	FUNCS->atomic_begin(crtc, old_crtc_state);
+	FUNCS->atomic_begin(crtc, old_state);
	...>
 }

@@
struct drm_crtc_helper_funcs *FUNCS;
identifier old_crtc_state, old_state;
identifier crtc;
identifier f;
@@

 f(struct drm_crtc_state *old_crtc_state)
 {
	...
 	struct drm_atomic_state *old_state = old_crtc_state->state;
	<...
-	FUNCS->atomic_flush(crtc, old_crtc_state);
+	FUNCS->atomic_flush(crtc, old_state);
	...>
 }

@@
struct drm_crtc_helper_funcs *FUNCS;
struct drm_crtc *crtc;
struct drm_crtc_state *crtc_state;
identifier dev, state;
identifier f;
@@

 f(struct drm_device *dev, struct drm_atomic_state *state, ...)
 {
	<...
-	FUNCS->atomic_begin(crtc, crtc_state);
+	FUNCS->atomic_begin(crtc, state);
	...>
 }

@@
struct drm_crtc_helper_funcs *FUNCS;
struct drm_crtc *crtc;
struct drm_crtc_state *crtc_state;
identifier dev, state;
identifier f;
@@

 f(struct drm_device *dev, struct drm_atomic_state *state, ...)
 {
	<...
-	FUNCS->atomic_flush(crtc, crtc_state);
+	FUNCS->atomic_flush(crtc, state);
	...>
 }

@@
identifier crtc, old_state;
@@

 struct drm_crtc_helper_funcs {
	...
-	void (*atomic_begin)(struct drm_crtc *crtc, struct drm_crtc_state *old_state);
+	void (*atomic_begin)(struct drm_crtc *crtc, struct drm_atomic_state *state);
	...
-	void (*atomic_flush)(struct drm_crtc *crtc, struct drm_crtc_state *old_state);
+	void (*atomic_flush)(struct drm_crtc *crtc, struct drm_atomic_state *state);
	...
}

@ crtc_atomic_func @
identifier helpers;
identifier func;
@@

(
static struct drm_crtc_helper_funcs helpers = {
	...,
	.atomic_begin = func,
	...,
};
|
static struct drm_crtc_helper_funcs helpers = {
	...,
	.atomic_flush = func,
	...,
};
)

@ ignores_old_state @
identifier crtc_atomic_func.func;
identifier crtc, old_state;
@@

void func(struct drm_crtc *crtc,
		struct drm_crtc_state *old_state)
{
	... when != old_state
}

@ adds_old_state depends on crtc_atomic_func && !ignores_old_state @
identifier crtc_atomic_func.func;
identifier crtc, old_state;
@@

void func(struct drm_crtc *crtc, struct drm_crtc_state *old_state)
{
+	struct drm_crtc_state *old_state = drm_atomic_get_old_crtc_state(state, crtc);
	...
}

@ depends on crtc_atomic_func @
identifier crtc_atomic_func.func;
expression E;
type T;
@@

void func(...)
{
	...
-	T state = E;
+	T crtc_state = E;
	<+...
-	state
+	crtc_state
	...+>

}

@ depends on crtc_atomic_func @
identifier crtc_atomic_func.func;
type T;
@@

void func(...)
{
	...
-	T state;
+	T crtc_state;
	<+...
-	state
+	crtc_state
	...+>

}

@@
identifier old_state;
identifier crtc;
@@

 void vc4_hvs_atomic_flush(struct drm_crtc *crtc,
-			   struct drm_crtc_state *old_state
+			   struct drm_atomic_state *state
			   )
{
+	struct drm_crtc_state *old_state = drm_atomic_get_old_crtc_state(state, crtc);
	...
}

@@
identifier old_state;
identifier crtc;
@@

 void vc4_hvs_atomic_flush(struct drm_crtc *crtc,
-			   struct drm_crtc_state *old_state
+			   struct drm_atomic_state *state
			   );

@@
identifier old_state;
identifier crtc;
@@

 void vmw_du_crtc_atomic_begin(struct drm_crtc *crtc,
-			   struct drm_crtc_state *old_state
+			   struct drm_atomic_state *state
			   )
{
	...
}

@@
identifier old_state;
identifier crtc;
@@

 void vmw_du_crtc_atomic_begin(struct drm_crtc *crtc,
-			   struct drm_crtc_state *old_state
+			   struct drm_atomic_state *state
			   );

@@
identifier old_state;
identifier crtc;
@@

 void vmw_du_crtc_atomic_flush(struct drm_crtc *crtc,
-			   struct drm_crtc_state *old_state
+			   struct drm_atomic_state *state
			   )
{
	...
}

@@
identifier old_state;
identifier crtc;
@@

 void vmw_du_crtc_atomic_flush(struct drm_crtc *crtc,
-			   struct drm_crtc_state *old_state
+			   struct drm_atomic_state *state
			   );

@ depends on crtc_atomic_func @
identifier crtc_atomic_func.func;
identifier old_state;
identifier crtc;
@@

void func(struct drm_crtc *crtc,
-	       struct drm_crtc_state *old_state
+	       struct drm_atomic_state *state
	       )
		{ ... }

@ include depends on adds_old_state @
@@

 #include <drm/drm_atomic.h>

@ no_include depends on !include && adds_old_state @
@@

+ #include <drm/drm_atomic.h>
  #include <drm/...>

Signed-off-by: Maxime Ripard <maxime@cerno.tech>
Reviewed-by: Ville Syrjälä <ville.syrjala@linux.intel.com>
Acked-by: Daniel Vetter <daniel.vetter@ffwll.ch>
Acked-by: Thomas Zimmermann <tzimmermann@suse.de>
Link: https://patchwork.freedesktop.org/patch/msgid/20201028123222.1732139-2-maxime@cerno.tech
---
 drivers/gpu/drm/arm/display/komeda/komeda_crtc.c |  4 +++-
 drivers/gpu/drm/arm/hdlcd_crtc.c                 |  2 +-
 drivers/gpu/drm/armada/armada_crtc.c             |  4 ++--
 drivers/gpu/drm/atmel-hlcdc/atmel_hlcdc_crtc.c   |  4 ++--
 drivers/gpu/drm/drm_atomic_helper.c              |  8 ++++----
 drivers/gpu/drm/exynos/exynos_drm_crtc.c         |  4 ++--
 drivers/gpu/drm/fsl-dcu/fsl_dcu_drm_crtc.c       |  2 +-
 drivers/gpu/drm/hisilicon/hibmc/hibmc_drm_de.c   |  4 ++--
 drivers/gpu/drm/hisilicon/kirin/kirin_drm_ade.c  |  4 ++--
 drivers/gpu/drm/imx/dcss/dcss-crtc.c             |  4 ++--
 drivers/gpu/drm/imx/ipuv3-crtc.c                 |  4 ++--
 drivers/gpu/drm/ingenic/ingenic-drm-drv.c        | 14 +++++++-------
 drivers/gpu/drm/mediatek/mtk_drm_crtc.c          | 16 ++++++++--------
 drivers/gpu/drm/meson/meson_crtc.c               |  4 ++--
 drivers/gpu/drm/msm/disp/dpu1/dpu_crtc.c         |  4 ++--
 drivers/gpu/drm/msm/disp/mdp4/mdp4_crtc.c        |  4 ++--
 drivers/gpu/drm/msm/disp/mdp5/mdp5_crtc.c        |  4 ++--
 drivers/gpu/drm/mxsfb/mxsfb_kms.c                |  2 +-
 drivers/gpu/drm/omapdrm/omap_crtc.c              |  4 ++--
 drivers/gpu/drm/qxl/qxl_display.c                |  2 +-
 drivers/gpu/drm/rcar-du/rcar_du_crtc.c           |  4 ++--
 drivers/gpu/drm/rockchip/rockchip_drm_vop.c      |  8 ++++++--
 drivers/gpu/drm/sti/sti_crtc.c                   |  2 +-
 drivers/gpu/drm/stm/ltdc.c                       |  2 +-
 drivers/gpu/drm/sun4i/sun4i_crtc.c               |  6 ++++--
 drivers/gpu/drm/tegra/dc.c                       | 10 +++++-----
 drivers/gpu/drm/tidss/tidss_crtc.c               |  4 +++-
 drivers/gpu/drm/tilcdc/tilcdc_crtc.c             |  2 +-
 drivers/gpu/drm/vboxvideo/vbox_mode.c            |  2 +-
 drivers/gpu/drm/vc4/vc4_drv.h                    |  3 ++-
 drivers/gpu/drm/vc4/vc4_hvs.c                    |  4 +++-
 drivers/gpu/drm/virtio/virtgpu_display.c         |  2 +-
 drivers/gpu/drm/vkms/vkms_crtc.c                 |  4 ++--
 drivers/gpu/drm/vmwgfx/vmwgfx_kms.c              |  4 ++--
 drivers/gpu/drm/vmwgfx/vmwgfx_kms.h              |  4 ++--
 drivers/gpu/drm/xlnx/zynqmp_disp.c               |  4 ++--
 drivers/gpu/drm/zte/zx_vou.c                     |  2 +-
 include/drm/drm_modeset_helper_vtables.h         |  4 ++--
 38 files changed, 91 insertions(+), 78 deletions(-)

--- a/drivers/gpu/drm/arm/display/komeda/komeda_crtc.c
+++ b/drivers/gpu/drm/arm/display/komeda/komeda_crtc.c
@@ -385,8 +385,10 @@ komeda_crtc_atomic_disable(struct drm_cr
 
 static void
 komeda_crtc_atomic_flush(struct drm_crtc *crtc,
-			 struct drm_crtc_state *old)
+			 struct drm_atomic_state *state)
 {
+	struct drm_crtc_state *old = drm_atomic_get_old_crtc_state(state,
+								   crtc);
 	/* commit with modeset will be handled in enable/disable */
 	if (drm_atomic_crtc_needs_modeset(crtc->state))
 		return;
--- a/drivers/gpu/drm/arm/hdlcd_crtc.c
+++ b/drivers/gpu/drm/arm/hdlcd_crtc.c
@@ -205,7 +205,7 @@ static enum drm_mode_status hdlcd_crtc_m
 }
 
 static void hdlcd_crtc_atomic_begin(struct drm_crtc *crtc,
-				    struct drm_crtc_state *state)
+				    struct drm_atomic_state *state)
 {
 	struct drm_pending_vblank_event *event = crtc->state->event;
 
--- a/drivers/gpu/drm/armada/armada_crtc.c
+++ b/drivers/gpu/drm/armada/armada_crtc.c
@@ -429,7 +429,7 @@ static int armada_drm_crtc_atomic_check(
 }
 
 static void armada_drm_crtc_atomic_begin(struct drm_crtc *crtc,
-					 struct drm_crtc_state *old_crtc_state)
+					 struct drm_atomic_state *state)
 {
 	struct armada_crtc *dcrtc = drm_to_armada_crtc(crtc);
 
@@ -443,7 +443,7 @@ static void armada_drm_crtc_atomic_begin
 }
 
 static void armada_drm_crtc_atomic_flush(struct drm_crtc *crtc,
-					 struct drm_crtc_state *old_crtc_state)
+					 struct drm_atomic_state *state)
 {
 	struct armada_crtc *dcrtc = drm_to_armada_crtc(crtc);
 
--- a/drivers/gpu/drm/atmel-hlcdc/atmel_hlcdc_crtc.c
+++ b/drivers/gpu/drm/atmel-hlcdc/atmel_hlcdc_crtc.c
@@ -342,7 +342,7 @@ static int atmel_hlcdc_crtc_atomic_check
 }
 
 static void atmel_hlcdc_crtc_atomic_begin(struct drm_crtc *c,
-					  struct drm_crtc_state *old_s)
+					  struct drm_atomic_state *state)
 {
 	struct atmel_hlcdc_crtc *crtc = drm_crtc_to_atmel_hlcdc_crtc(c);
 
@@ -357,7 +357,7 @@ static void atmel_hlcdc_crtc_atomic_begi
 }
 
 static void atmel_hlcdc_crtc_atomic_flush(struct drm_crtc *crtc,
-					  struct drm_crtc_state *old_s)
+					  struct drm_atomic_state *state)
 {
 	/* TODO: write common plane control register if available */
 }
--- a/drivers/gpu/drm/drm_atomic_helper.c
+++ b/drivers/gpu/drm/drm_atomic_helper.c
@@ -2517,7 +2517,7 @@ void drm_atomic_helper_commit_planes(str
 		if (active_only && !new_crtc_state->active)
 			continue;
 
-		funcs->atomic_begin(crtc, old_crtc_state);
+		funcs->atomic_begin(crtc, old_state);
 	}
 
 	for_each_oldnew_plane_in_state(old_state, plane, old_plane_state, new_plane_state, i) {
@@ -2575,7 +2575,7 @@ void drm_atomic_helper_commit_planes(str
 		if (active_only && !new_crtc_state->active)
 			continue;
 
-		funcs->atomic_flush(crtc, old_crtc_state);
+		funcs->atomic_flush(crtc, old_state);
 	}
 }
 EXPORT_SYMBOL(drm_atomic_helper_commit_planes);
@@ -2613,7 +2613,7 @@ drm_atomic_helper_commit_planes_on_crtc(
 
 	crtc_funcs = crtc->helper_private;
 	if (crtc_funcs && crtc_funcs->atomic_begin)
-		crtc_funcs->atomic_begin(crtc, old_crtc_state);
+		crtc_funcs->atomic_begin(crtc, old_state);
 
 	drm_for_each_plane_mask(plane, crtc->dev, plane_mask) {
 		struct drm_plane_state *old_plane_state =
@@ -2639,7 +2639,7 @@ drm_atomic_helper_commit_planes_on_crtc(
 	}
 
 	if (crtc_funcs && crtc_funcs->atomic_flush)
-		crtc_funcs->atomic_flush(crtc, old_crtc_state);
+		crtc_funcs->atomic_flush(crtc, old_state);
 }
 EXPORT_SYMBOL(drm_atomic_helper_commit_planes_on_crtc);
 
--- a/drivers/gpu/drm/exynos/exynos_drm_crtc.c
+++ b/drivers/gpu/drm/exynos/exynos_drm_crtc.c
@@ -65,7 +65,7 @@ static int exynos_crtc_atomic_check(stru
 }
 
 static void exynos_crtc_atomic_begin(struct drm_crtc *crtc,
-				     struct drm_crtc_state *old_crtc_state)
+				     struct drm_atomic_state *state)
 {
 	struct exynos_drm_crtc *exynos_crtc = to_exynos_crtc(crtc);
 
@@ -74,7 +74,7 @@ static void exynos_crtc_atomic_begin(str
 }
 
 static void exynos_crtc_atomic_flush(struct drm_crtc *crtc,
-				     struct drm_crtc_state *old_crtc_state)
+				     struct drm_atomic_state *state)
 {
 	struct exynos_drm_crtc *exynos_crtc = to_exynos_crtc(crtc);
 
--- a/drivers/gpu/drm/fsl-dcu/fsl_dcu_drm_crtc.c
+++ b/drivers/gpu/drm/fsl-dcu/fsl_dcu_drm_crtc.c
@@ -21,7 +21,7 @@
 #include "fsl_dcu_drm_plane.h"
 
 static void fsl_dcu_drm_crtc_atomic_flush(struct drm_crtc *crtc,
-					  struct drm_crtc_state *old_crtc_state)
+					  struct drm_atomic_state *state)
 {
 	struct drm_device *dev = crtc->dev;
 	struct fsl_dcu_drm_device *fsl_dev = dev->dev_private;
--- a/drivers/gpu/drm/hisilicon/hibmc/hibmc_drm_de.c
+++ b/drivers/gpu/drm/hisilicon/hibmc/hibmc_drm_de.c
@@ -393,7 +393,7 @@ static void hibmc_crtc_mode_set_nofb(str
 }
 
 static void hibmc_crtc_atomic_begin(struct drm_crtc *crtc,
-				    struct drm_crtc_state *old_state)
+				    struct drm_atomic_state *state)
 {
 	unsigned int reg;
 	struct drm_device *dev = crtc->dev;
@@ -413,7 +413,7 @@ static void hibmc_crtc_atomic_begin(stru
 }
 
 static void hibmc_crtc_atomic_flush(struct drm_crtc *crtc,
-				    struct drm_crtc_state *old_state)
+				    struct drm_atomic_state *state)
 
 {
 	unsigned long flags;
--- a/drivers/gpu/drm/hisilicon/kirin/kirin_drm_ade.c
+++ b/drivers/gpu/drm/hisilicon/kirin/kirin_drm_ade.c
@@ -485,7 +485,7 @@ static void ade_crtc_mode_set_nofb(struc
 }
 
 static void ade_crtc_atomic_begin(struct drm_crtc *crtc,
-				  struct drm_crtc_state *old_state)
+				  struct drm_atomic_state *state)
 {
 	struct kirin_crtc *kcrtc = to_kirin_crtc(crtc);
 	struct ade_hw_ctx *ctx = kcrtc->hw_ctx;
@@ -498,7 +498,7 @@ static void ade_crtc_atomic_begin(struct
 }
 
 static void ade_crtc_atomic_flush(struct drm_crtc *crtc,
-				  struct drm_crtc_state *old_state)
+				  struct drm_atomic_state *state)
 
 {
 	struct kirin_crtc *kcrtc = to_kirin_crtc(crtc);
--- a/drivers/gpu/drm/imx/dcss/dcss-crtc.c
+++ b/drivers/gpu/drm/imx/dcss/dcss-crtc.c
@@ -53,13 +53,13 @@ static const struct drm_crtc_funcs dcss_
 };
 
 static void dcss_crtc_atomic_begin(struct drm_crtc *crtc,
-				   struct drm_crtc_state *old_crtc_state)
+				   struct drm_atomic_state *state)
 {
 	drm_crtc_vblank_on(crtc);
 }
 
 static void dcss_crtc_atomic_flush(struct drm_crtc *crtc,
-				   struct drm_crtc_state *old_crtc_state)
+				   struct drm_atomic_state *state)
 {
 	struct dcss_crtc *dcss_crtc = container_of(crtc, struct dcss_crtc,
 						   base);
--- a/drivers/gpu/drm/imx/ipuv3-crtc.c
+++ b/drivers/gpu/drm/imx/ipuv3-crtc.c
@@ -240,13 +240,13 @@ static int ipu_crtc_atomic_check(struct
 }
 
 static void ipu_crtc_atomic_begin(struct drm_crtc *crtc,
-				  struct drm_crtc_state *old_crtc_state)
+				  struct drm_atomic_state *state)
 {
 	drm_crtc_vblank_on(crtc);
 }
 
 static void ipu_crtc_atomic_flush(struct drm_crtc *crtc,
-				  struct drm_crtc_state *old_crtc_state)
+				  struct drm_atomic_state *state)
 {
 	spin_lock_irq(&crtc->dev->event_lock);
 	if (crtc->state->event) {
--- a/drivers/gpu/drm/ingenic/ingenic-drm-drv.c
+++ b/drivers/gpu/drm/ingenic/ingenic-drm-drv.c
@@ -292,7 +292,7 @@ ingenic_drm_crtc_mode_valid(struct drm_c
 }
 
 static void ingenic_drm_crtc_atomic_begin(struct drm_crtc *crtc,
-					  struct drm_crtc_state *oldstate)
+					  struct drm_atomic_state *state)
 {
 	struct ingenic_drm *priv = drm_crtc_get_priv(crtc);
 	u32 ctrl = 0;
@@ -312,26 +312,26 @@ static void ingenic_drm_crtc_atomic_begi
 }
 
 static void ingenic_drm_crtc_atomic_flush(struct drm_crtc *crtc,
-					  struct drm_crtc_state *oldstate)
+					  struct drm_atomic_state *state)
 {
 	struct ingenic_drm *priv = drm_crtc_get_priv(crtc);
-	struct drm_crtc_state *state = crtc->state;
-	struct drm_pending_vblank_event *event = state->event;
+	struct drm_crtc_state *crtc_state = crtc->state;
+	struct drm_pending_vblank_event *event = crtc_state->event;
 
-	if (drm_atomic_crtc_needs_modeset(state)) {
+	if (drm_atomic_crtc_needs_modeset(crtc_state)) {
 		ingenic_drm_crtc_update_timings(priv, &state->mode);
 		priv->update_clk_rate = true;
 	}
 
 	if (priv->update_clk_rate) {
 		mutex_lock(&priv->clk_mutex);
-		clk_set_rate(priv->pix_clk, state->adjusted_mode.clock * 1000);
+		clk_set_rate(priv->pix_clk, crtc_state->adjusted_mode.clock * 1000);
 		priv->update_clk_rate = false;
 		mutex_unlock(&priv->clk_mutex);
 	}
 
 	if (event) {
-		state->event = NULL;
+		crtc_state->event = NULL;
 
 		spin_lock_irq(&crtc->dev->event_lock);
 		if (drm_crtc_vblank_get(crtc) == 0)
--- a/drivers/gpu/drm/mediatek/mtk_drm_crtc.c
+++ b/drivers/gpu/drm/mediatek/mtk_drm_crtc.c
@@ -575,24 +575,24 @@ static void mtk_drm_crtc_atomic_disable(
 }
 
 static void mtk_drm_crtc_atomic_begin(struct drm_crtc *crtc,
-				      struct drm_crtc_state *old_crtc_state)
+				      struct drm_atomic_state *state)
 {
-	struct mtk_crtc_state *state = to_mtk_crtc_state(crtc->state);
+	struct mtk_crtc_state *crtc_state = to_mtk_crtc_state(crtc->state);
 	struct mtk_drm_crtc *mtk_crtc = to_mtk_crtc(crtc);
 
-	if (mtk_crtc->event && state->base.event)
+	if (mtk_crtc->event && crtc_state->base.event)
 		DRM_ERROR("new event while there is still a pending event\n");
 
-	if (state->base.event) {
-		state->base.event->pipe = drm_crtc_index(crtc);
+	if (crtc_state->base.event) {
+		crtc_state->base.event->pipe = drm_crtc_index(crtc);
 		WARN_ON(drm_crtc_vblank_get(crtc) != 0);
-		mtk_crtc->event = state->base.event;
-		state->base.event = NULL;
+		mtk_crtc->event = crtc_state->base.event;
+		crtc_state->base.event = NULL;
 	}
 }
 
 static void mtk_drm_crtc_atomic_flush(struct drm_crtc *crtc,
-				      struct drm_crtc_state *old_crtc_state)
+				      struct drm_atomic_state *state)
 {
 	struct mtk_drm_crtc *mtk_crtc = to_mtk_crtc(crtc);
 	int i;
--- a/drivers/gpu/drm/meson/meson_crtc.c
+++ b/drivers/gpu/drm/meson/meson_crtc.c
@@ -201,7 +201,7 @@ static void meson_crtc_atomic_disable(st
 }
 
 static void meson_crtc_atomic_begin(struct drm_crtc *crtc,
-				    struct drm_crtc_state *state)
+				    struct drm_atomic_state *state)
 {
 	struct meson_crtc *meson_crtc = to_meson_crtc(crtc);
 	unsigned long flags;
@@ -217,7 +217,7 @@ static void meson_crtc_atomic_begin(stru
 }
 
 static void meson_crtc_atomic_flush(struct drm_crtc *crtc,
-				    struct drm_crtc_state *old_crtc_state)
+				    struct drm_atomic_state *state)
 {
 	struct meson_crtc *meson_crtc = to_meson_crtc(crtc);
 	struct meson_drm *priv = meson_crtc->priv;
--- a/drivers/gpu/drm/msm/disp/dpu1/dpu_crtc.c
+++ b/drivers/gpu/drm/msm/disp/dpu1/dpu_crtc.c
@@ -486,7 +486,7 @@ static void _dpu_crtc_setup_cp_blocks(st
 }
 
 static void dpu_crtc_atomic_begin(struct drm_crtc *crtc,
-		struct drm_crtc_state *old_state)
+		struct drm_atomic_state *state)
 {
 	struct dpu_crtc_state *cstate = to_dpu_crtc_state(crtc->state);
 	struct drm_encoder *encoder;
@@ -527,7 +527,7 @@ static void dpu_crtc_atomic_begin(struct
 }
 
 static void dpu_crtc_atomic_flush(struct drm_crtc *crtc,
-		struct drm_crtc_state *old_crtc_state)
+		struct drm_atomic_state *state)
 {
 	struct dpu_crtc *dpu_crtc;
 	struct drm_device *dev;
--- a/drivers/gpu/drm/msm/disp/mdp4/mdp4_crtc.c
+++ b/drivers/gpu/drm/msm/disp/mdp4/mdp4_crtc.c
@@ -316,14 +316,14 @@ static int mdp4_crtc_atomic_check(struct
 }
 
 static void mdp4_crtc_atomic_begin(struct drm_crtc *crtc,
-				   struct drm_crtc_state *old_crtc_state)
+				   struct drm_atomic_state *state)
 {
 	struct mdp4_crtc *mdp4_crtc = to_mdp4_crtc(crtc);
 	DBG("%s: begin", mdp4_crtc->name);
 }
 
 static void mdp4_crtc_atomic_flush(struct drm_crtc *crtc,
-				   struct drm_crtc_state *old_crtc_state)
+				   struct drm_atomic_state *state)
 {
 	struct mdp4_crtc *mdp4_crtc = to_mdp4_crtc(crtc);
 	struct drm_device *dev = crtc->dev;
--- a/drivers/gpu/drm/msm/disp/mdp5/mdp5_crtc.c
+++ b/drivers/gpu/drm/msm/disp/mdp5/mdp5_crtc.c
@@ -778,13 +778,13 @@ static int mdp5_crtc_atomic_check(struct
 }
 
 static void mdp5_crtc_atomic_begin(struct drm_crtc *crtc,
-				   struct drm_crtc_state *old_crtc_state)
+				   struct drm_atomic_state *state)
 {
 	DBG("%s: begin", crtc->name);
 }
 
 static void mdp5_crtc_atomic_flush(struct drm_crtc *crtc,
-				   struct drm_crtc_state *old_crtc_state)
+				   struct drm_atomic_state *state)
 {
 	struct mdp5_crtc *mdp5_crtc = to_mdp5_crtc(crtc);
 	struct mdp5_crtc_state *mdp5_cstate = to_mdp5_crtc_state(crtc->state);
--- a/drivers/gpu/drm/mxsfb/mxsfb_kms.c
+++ b/drivers/gpu/drm/mxsfb/mxsfb_kms.c
@@ -326,7 +326,7 @@ static int mxsfb_crtc_atomic_check(struc
 }
 
 static void mxsfb_crtc_atomic_flush(struct drm_crtc *crtc,
-				    struct drm_crtc_state *old_state)
+				    struct drm_atomic_state *state)
 {
 	struct drm_pending_vblank_event *event;
 
--- a/drivers/gpu/drm/omapdrm/omap_crtc.c
+++ b/drivers/gpu/drm/omapdrm/omap_crtc.c
@@ -601,12 +601,12 @@ static int omap_crtc_atomic_check(struct
 }
 
 static void omap_crtc_atomic_begin(struct drm_crtc *crtc,
-				   struct drm_crtc_state *old_crtc_state)
+				   struct drm_atomic_state *state)
 {
 }
 
 static void omap_crtc_atomic_flush(struct drm_crtc *crtc,
-				   struct drm_crtc_state *old_crtc_state)
+				   struct drm_atomic_state *state)
 {
 	struct omap_drm_private *priv = crtc->dev->dev_private;
 	struct omap_crtc *omap_crtc = to_omap_crtc(crtc);
--- a/drivers/gpu/drm/qxl/qxl_display.c
+++ b/drivers/gpu/drm/qxl/qxl_display.c
@@ -373,7 +373,7 @@ static void qxl_crtc_update_monitors_con
 }
 
 static void qxl_crtc_atomic_flush(struct drm_crtc *crtc,
-				  struct drm_crtc_state *old_crtc_state)
+				  struct drm_atomic_state *state)
 {
 	qxl_crtc_update_monitors_config(crtc, "flush");
 }
--- a/drivers/gpu/drm/rcar-du/rcar_du_crtc.c
+++ b/drivers/gpu/drm/rcar-du/rcar_du_crtc.c
@@ -785,7 +785,7 @@ static void rcar_du_crtc_atomic_disable(
 }
 
 static void rcar_du_crtc_atomic_begin(struct drm_crtc *crtc,
-				      struct drm_crtc_state *old_crtc_state)
+				      struct drm_atomic_state *state)
 {
 	struct rcar_du_crtc *rcrtc = to_rcar_crtc(crtc);
 
@@ -814,7 +814,7 @@ static void rcar_du_crtc_atomic_begin(st
 }
 
 static void rcar_du_crtc_atomic_flush(struct drm_crtc *crtc,
-				      struct drm_crtc_state *old_crtc_state)
+				      struct drm_atomic_state *state)
 {
 	struct rcar_du_crtc *rcrtc = to_rcar_crtc(crtc);
 	struct drm_device *dev = rcrtc->crtc.dev;
--- a/drivers/gpu/drm/rockchip/rockchip_drm_vop.c
+++ b/drivers/gpu/drm/rockchip/rockchip_drm_vop.c
@@ -1247,8 +1247,10 @@ static void vop_crtc_gamma_set(struct vo
 }
 
 static void vop_crtc_atomic_begin(struct drm_crtc *crtc,
-				  struct drm_crtc_state *old_crtc_state)
+				  struct drm_atomic_state *state)
 {
+	struct drm_crtc_state *old_crtc_state = drm_atomic_get_old_crtc_state(state,
+									      crtc);
 	struct vop *vop = to_vop(crtc);
 
 	/*
@@ -1463,8 +1465,10 @@ static int vop_crtc_atomic_check(struct
 }
 
 static void vop_crtc_atomic_flush(struct drm_crtc *crtc,
-				  struct drm_crtc_state *old_crtc_state)
+				  struct drm_atomic_state *state)
 {
+	struct drm_crtc_state *old_crtc_state = drm_atomic_get_old_crtc_state(state,
+									      crtc);
 	struct drm_atomic_state *old_state = old_crtc_state->state;
 	struct drm_plane_state *old_plane_state, *new_plane_state;
 	struct vop *vop = to_vop(crtc);
--- a/drivers/gpu/drm/sti/sti_crtc.c
+++ b/drivers/gpu/drm/sti/sti_crtc.c
@@ -133,7 +133,7 @@ sti_crtc_mode_set_nofb(struct drm_crtc *
 }
 
 static void sti_crtc_atomic_flush(struct drm_crtc *crtc,
-				  struct drm_crtc_state *old_crtc_state)
+				  struct drm_atomic_state *state)
 {
 	struct drm_device *drm_dev = crtc->dev;
 	struct sti_mixer *mixer = to_sti_mixer(crtc);
--- a/drivers/gpu/drm/stm/ltdc.c
+++ b/drivers/gpu/drm/stm/ltdc.c
@@ -629,7 +629,7 @@ static void ltdc_crtc_mode_set_nofb(stru
 }
 
 static void ltdc_crtc_atomic_flush(struct drm_crtc *crtc,
-				   struct drm_crtc_state *old_crtc_state)
+				   struct drm_atomic_state *state)
 {
 	struct ltdc_device *ldev = crtc_to_ltdc(crtc);
 	struct drm_device *ddev = crtc->dev;
--- a/drivers/gpu/drm/sun4i/sun4i_crtc.c
+++ b/drivers/gpu/drm/sun4i/sun4i_crtc.c
@@ -61,8 +61,10 @@ static int sun4i_crtc_atomic_check(struc
 }
 
 static void sun4i_crtc_atomic_begin(struct drm_crtc *crtc,
-				    struct drm_crtc_state *old_state)
+				    struct drm_atomic_state *state)
 {
+	struct drm_crtc_state *old_state = drm_atomic_get_old_crtc_state(state,
+									 crtc);
 	struct sun4i_crtc *scrtc = drm_crtc_to_sun4i_crtc(crtc);
 	struct drm_device *dev = crtc->dev;
 	struct sunxi_engine *engine = scrtc->engine;
@@ -82,7 +84,7 @@ static void sun4i_crtc_atomic_begin(stru
 }
 
 static void sun4i_crtc_atomic_flush(struct drm_crtc *crtc,
-				    struct drm_crtc_state *old_state)
+				    struct drm_atomic_state *state)
 {
 	struct sun4i_crtc *scrtc = drm_crtc_to_sun4i_crtc(crtc);
 	struct drm_pending_vblank_event *event = crtc->state->event;
--- a/drivers/gpu/drm/tegra/dc.c
+++ b/drivers/gpu/drm/tegra/dc.c
@@ -1924,7 +1924,7 @@ static void tegra_crtc_atomic_enable(str
 }
 
 static void tegra_crtc_atomic_begin(struct drm_crtc *crtc,
-				    struct drm_crtc_state *old_crtc_state)
+				    struct drm_atomic_state *state)
 {
 	unsigned long flags;
 
@@ -1943,17 +1943,17 @@ static void tegra_crtc_atomic_begin(stru
 }
 
 static void tegra_crtc_atomic_flush(struct drm_crtc *crtc,
-				    struct drm_crtc_state *old_crtc_state)
+				    struct drm_atomic_state *state)
 {
-	struct tegra_dc_state *state = to_dc_state(crtc->state);
+	struct tegra_dc_state *crtc_state = to_dc_state(crtc->state);
 	struct tegra_dc *dc = to_tegra_dc(crtc);
 	u32 value;
 
-	value = state->planes << 8 | GENERAL_UPDATE;
+	value = crtc_state->planes << 8 | GENERAL_UPDATE;
 	tegra_dc_writel(dc, value, DC_CMD_STATE_CONTROL);
 	value = tegra_dc_readl(dc, DC_CMD_STATE_CONTROL);
 
-	value = state->planes | GENERAL_ACT_REQ;
+	value = crtc_state->planes | GENERAL_ACT_REQ;
 	tegra_dc_writel(dc, value, DC_CMD_STATE_CONTROL);
 	value = tegra_dc_readl(dc, DC_CMD_STATE_CONTROL);
 }
--- a/drivers/gpu/drm/tidss/tidss_crtc.c
+++ b/drivers/gpu/drm/tidss/tidss_crtc.c
@@ -163,8 +163,10 @@ static void tidss_crtc_position_planes(s
 }
 
 static void tidss_crtc_atomic_flush(struct drm_crtc *crtc,
-				    struct drm_crtc_state *old_crtc_state)
+				    struct drm_atomic_state *state)
 {
+	struct drm_crtc_state *old_crtc_state = drm_atomic_get_old_crtc_state(state,
+									      crtc);
 	struct tidss_crtc *tcrtc = to_tidss_crtc(crtc);
 	struct drm_device *ddev = crtc->dev;
 	struct tidss_device *tidss = to_tidss(ddev);
--- a/drivers/gpu/drm/tilcdc/tilcdc_crtc.c
+++ b/drivers/gpu/drm/tilcdc/tilcdc_crtc.c
@@ -547,7 +547,7 @@ static void tilcdc_crtc_atomic_disable(s
 }
 
 static void tilcdc_crtc_atomic_flush(struct drm_crtc *crtc,
-				     struct drm_crtc_state *old_state)
+				     struct drm_atomic_state *state)
 {
 	if (!crtc->state->event)
 		return;
--- a/drivers/gpu/drm/vboxvideo/vbox_mode.c
+++ b/drivers/gpu/drm/vboxvideo/vbox_mode.c
@@ -223,7 +223,7 @@ static void vbox_crtc_atomic_disable(str
 }
 
 static void vbox_crtc_atomic_flush(struct drm_crtc *crtc,
-				   struct drm_crtc_state *old_crtc_state)
+				   struct drm_atomic_state *state)
 {
 }
 
--- a/drivers/gpu/drm/vc4/vc4_drv.h
+++ b/drivers/gpu/drm/vc4/vc4_drv.h
@@ -928,7 +928,8 @@ int vc4_hvs_get_fifo_from_output(struct
 int vc4_hvs_atomic_check(struct drm_crtc *crtc, struct drm_crtc_state *state);
 void vc4_hvs_atomic_enable(struct drm_crtc *crtc, struct drm_crtc_state *old_state);
 void vc4_hvs_atomic_disable(struct drm_crtc *crtc, struct drm_crtc_state *old_state);
-void vc4_hvs_atomic_flush(struct drm_crtc *crtc, struct drm_crtc_state *state);
+void vc4_hvs_atomic_flush(struct drm_crtc *crtc,
+			  struct drm_atomic_state *state);
 void vc4_hvs_dump_state(struct drm_device *dev);
 void vc4_hvs_unmask_underrun(struct drm_device *dev, int channel);
 void vc4_hvs_mask_underrun(struct drm_device *dev, int channel);
--- a/drivers/gpu/drm/vc4/vc4_hvs.c
+++ b/drivers/gpu/drm/vc4/vc4_hvs.c
@@ -453,8 +453,10 @@ void vc4_hvs_atomic_disable(struct drm_c
 }
 
 void vc4_hvs_atomic_flush(struct drm_crtc *crtc,
-			  struct drm_crtc_state *old_state)
+			  struct drm_atomic_state *state)
 {
+	struct drm_crtc_state *old_state = drm_atomic_get_old_crtc_state(state,
+									 crtc);
 	struct drm_device *dev = crtc->dev;
 	struct vc4_dev *vc4 = to_vc4_dev(dev);
 	struct vc4_crtc_state *vc4_state = to_vc4_crtc_state(crtc->state);
--- a/drivers/gpu/drm/virtio/virtgpu_display.c
+++ b/drivers/gpu/drm/virtio/virtgpu_display.c
@@ -117,7 +117,7 @@ static int virtio_gpu_crtc_atomic_check(
 }
 
 static void virtio_gpu_crtc_atomic_flush(struct drm_crtc *crtc,
-					 struct drm_crtc_state *old_state)
+					 struct drm_atomic_state *state)
 {
 	struct virtio_gpu_output *output = drm_crtc_to_virtio_gpu_output(crtc);
 
--- a/drivers/gpu/drm/vkms/vkms_crtc.c
+++ b/drivers/gpu/drm/vkms/vkms_crtc.c
@@ -229,7 +229,7 @@ static void vkms_crtc_atomic_disable(str
 }
 
 static void vkms_crtc_atomic_begin(struct drm_crtc *crtc,
-				   struct drm_crtc_state *old_crtc_state)
+				   struct drm_atomic_state *state)
 {
 	struct vkms_output *vkms_output = drm_crtc_to_vkms_output(crtc);
 
@@ -240,7 +240,7 @@ static void vkms_crtc_atomic_begin(struc
 }
 
 static void vkms_crtc_atomic_flush(struct drm_crtc *crtc,
-				   struct drm_crtc_state *old_crtc_state)
+				   struct drm_atomic_state *state)
 {
 	struct vkms_output *vkms_output = drm_crtc_to_vkms_output(crtc);
 
--- a/drivers/gpu/drm/vmwgfx/vmwgfx_kms.c
+++ b/drivers/gpu/drm/vmwgfx/vmwgfx_kms.c
@@ -554,13 +554,13 @@ int vmw_du_crtc_atomic_check(struct drm_
 
 
 void vmw_du_crtc_atomic_begin(struct drm_crtc *crtc,
-			      struct drm_crtc_state *old_crtc_state)
+			      struct drm_atomic_state *state)
 {
 }
 
 
 void vmw_du_crtc_atomic_flush(struct drm_crtc *crtc,
-			      struct drm_crtc_state *old_crtc_state)
+			      struct drm_atomic_state *state)
 {
 	struct drm_pending_vblank_event *event = crtc->state->event;
 
--- a/drivers/gpu/drm/vmwgfx/vmwgfx_kms.h
+++ b/drivers/gpu/drm/vmwgfx/vmwgfx_kms.h
@@ -475,9 +475,9 @@ void vmw_du_plane_unpin_surf(struct vmw_
 int vmw_du_crtc_atomic_check(struct drm_crtc *crtc,
 			     struct drm_atomic_state *state);
 void vmw_du_crtc_atomic_begin(struct drm_crtc *crtc,
-			      struct drm_crtc_state *old_crtc_state);
+			      struct drm_atomic_state *state);
 void vmw_du_crtc_atomic_flush(struct drm_crtc *crtc,
-			      struct drm_crtc_state *old_crtc_state);
+			      struct drm_atomic_state *state);
 void vmw_du_crtc_reset(struct drm_crtc *crtc);
 struct drm_crtc_state *vmw_du_crtc_duplicate_state(struct drm_crtc *crtc);
 void vmw_du_crtc_destroy_state(struct drm_crtc *crtc,
--- a/drivers/gpu/drm/xlnx/zynqmp_disp.c
+++ b/drivers/gpu/drm/xlnx/zynqmp_disp.c
@@ -1515,14 +1515,14 @@ static int zynqmp_disp_crtc_atomic_check
 
 static void
 zynqmp_disp_crtc_atomic_begin(struct drm_crtc *crtc,
-			      struct drm_crtc_state *old_crtc_state)
+			      struct drm_atomic_state *state)
 {
 	drm_crtc_vblank_on(crtc);
 }
 
 static void
 zynqmp_disp_crtc_atomic_flush(struct drm_crtc *crtc,
-			      struct drm_crtc_state *old_crtc_state)
+			      struct drm_atomic_state *state)
 {
 	if (crtc->state->event) {
 		struct drm_pending_vblank_event *event;
--- a/drivers/gpu/drm/zte/zx_vou.c
+++ b/drivers/gpu/drm/zte/zx_vou.c
@@ -473,7 +473,7 @@ static void zx_crtc_atomic_disable(struc
 }
 
 static void zx_crtc_atomic_flush(struct drm_crtc *crtc,
-				  struct drm_crtc_state *old_state)
+				  struct drm_atomic_state *state)
 {
 	struct drm_pending_vblank_event *event = crtc->state->event;
 
--- a/include/drm/drm_modeset_helper_vtables.h
+++ b/include/drm/drm_modeset_helper_vtables.h
@@ -373,7 +373,7 @@ struct drm_crtc_helper_funcs {
 	 * transitional plane helpers, but it is optional.
 	 */
 	void (*atomic_begin)(struct drm_crtc *crtc,
-			     struct drm_crtc_state *old_crtc_state);
+			     struct drm_atomic_state *state);
 	/**
 	 * @atomic_flush:
 	 *
@@ -397,7 +397,7 @@ struct drm_crtc_helper_funcs {
 	 * transitional plane helpers, but it is optional.
 	 */
 	void (*atomic_flush)(struct drm_crtc *crtc,
-			     struct drm_crtc_state *old_crtc_state);
+			     struct drm_atomic_state *state);
 
 	/**
 	 * @atomic_enable:
