From 20534fd2fedd5c3febd239475e64d3dfc7d8400b Mon Sep 17 00:00:00 2001
From: Stefan Wahren <wahrenst@gmx.net>
Date: Fri, 27 Dec 2019 11:40:56 +0100
Subject: [PATCH] ARM: bcm: Backport BCM2711 support from upstream

Make the BCM2711 a different machine, but keep it in board_bcm2835.

Signed-off-by: Stefan Wahren <wahrenst@gmx.net>
---
 arch/arm/mach-bcm/board_bcm2835.c | 17 +++++++++++++++--
 1 file changed, 15 insertions(+), 2 deletions(-)

--- a/arch/arm/mach-bcm/board_bcm2835.c
+++ b/arch/arm/mach-bcm/board_bcm2835.c
@@ -109,17 +109,30 @@ static const char * const bcm2835_compat
 #ifdef CONFIG_ARCH_MULTI_V7
 	"brcm,bcm2836",
 	"brcm,bcm2837",
-	"brcm,bcm2711",
 #endif
 	NULL
 };
 
 DT_MACHINE_START(BCM2835, "BCM2835")
+	.map_io = bcm2835_map_io,
+	.init_machine = bcm2835_init,
+	.dt_compat = bcm2835_compat,
+	.smp = smp_ops(bcm2836_smp_ops),
+MACHINE_END
+
+static const char * const bcm2711_compat[] = {
+#ifdef CONFIG_ARCH_MULTI_V7
+	"brcm,bcm2711",
+#endif
+	NULL
+};
+
+DT_MACHINE_START(BCM2711, "BCM2711")
 #if defined(CONFIG_ZONE_DMA) && defined(CONFIG_ARM_LPAE)
 	.dma_zone_size	= SZ_1G,
 #endif
 	.map_io = bcm2835_map_io,
 	.init_machine = bcm2835_init,
-	.dt_compat = bcm2835_compat,
+	.dt_compat = bcm2711_compat,
 	.smp = smp_ops(bcm2836_smp_ops),
 MACHINE_END
