From 68eabc348148ae051631e8dab13c3b1a85c82896 Mon Sep 17 00:00:00 2001
From: Aleksander Jan Bajkowski <olek2@wp.pl>
Date: Tue, 9 Nov 2021 23:23:54 +0100
Subject: [PATCH] net: ethernet: lantiq_etop: Fix compilation error

This fixes the error detected when compiling the driver.

Fixes: 14d4e308e0aa ("net: lantiq: configure the burst length in ethernet drivers")
Reported-by: kernel test robot <lkp@intel.com>
Signed-off-by: Aleksander Jan Bajkowski <olek2@wp.pl>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/ethernet/lantiq_etop.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/net/ethernet/lantiq_etop.c
+++ b/drivers/net/ethernet/lantiq_etop.c
@@ -402,7 +402,7 @@ ltq_etop_dma_init(struct net_device *dev
 	int rx = priv->rx_irq - LTQ_DMA_ETOP;
 	int err;
 
-	ltq_dma_init_port(DMA_PORT_ETOP, priv->tx_burst_len, rx_burst_len);
+	ltq_dma_init_port(DMA_PORT_ETOP, priv->tx_burst_len, priv->rx_burst_len);
 
 	priv->txch.dma.nr = tx;
 	priv->txch.dma.dev = &priv->pdev->dev;
