From 89a7202785673e8bcef072ebcbe1eb0599b8ba88 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.com>
Date: Mon, 15 Feb 2021 10:32:18 +0000
Subject: [PATCH] overlays: Rename gpio-fsm property num-soft-gpios

The gpio-fsm property "num-soft-gpios" triggers a kernel DT checker
that warns about the lack of #gpio-cells on a random node with the
phandle that just happens to match the number of soft GPIOs. Rename
the property to "num-swgpios" to avoid the warning.

Signed-off-by: Phil Elwell <phil@raspberrypi.com>
---
 arch/arm/boot/dts/overlays/fsm-demo-overlay.dts  | 2 +-
 arch/arm/boot/dts/overlays/ghost-amp-overlay.dts | 2 +-
 2 files changed, 2 insertions(+), 2 deletions(-)

--- a/arch/arm/boot/dts/overlays/fsm-demo-overlay.dts
+++ b/arch/arm/boot/dts/overlays/fsm-demo-overlay.dts
@@ -22,7 +22,7 @@
 				debug = <0>;
 				gpio-controller;
 				#gpio-cells = <2>;
-				num-soft-gpios = <1>;
+				num-swgpios = <1>;
 				gpio-line-names = "button2";
 				input-gpios  = <&gpio 6 1>;  // BUTTON1 (active-low)
 				output-gpios = <&gpio 7 0>,  // RED
--- a/arch/arm/boot/dts/overlays/ghost-amp-overlay.dts
+++ b/arch/arm/boot/dts/overlays/ghost-amp-overlay.dts
@@ -58,7 +58,7 @@
 				debug = <0>;
 				gpio-controller;
 				#gpio-cells = <2>;
-				num-soft-gpios = <1>;
+				num-swgpios = <1>;
 				gpio-line-names = "enable";
 				input-gpios  = <&gpio 5 1>;  // FAULT (active low)
 				output-gpios = <&gpio 22 0>, // RELAY1
