From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Mon, 18 Jul 2022 13:17:57 +0200
Subject: [PATCH] arm64: dts: broadcom: bcm4908: add LEDs controller block
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

BCM4908 includes LEDs controller that supports multiple brightness
levels & hardware blinking.

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
---
 arch/arm64/boot/dts/broadcom/bcm4908/bcm4908.dtsi | 8 ++++++++
 1 file changed, 8 insertions(+)

--- a/arch/arm64/boot/dts/broadcom/bcm4908/bcm4908.dtsi
+++ b/arch/arm64/boot/dts/broadcom/bcm4908/bcm4908.dtsi
@@ -517,6 +517,14 @@
 			status = "okay";
 		};
 
+		leds: leds@800 {
+			compatible = "brcm,bcm4908-leds", "brcm,bcm63138-leds";
+			reg = <0x800 0xdc>;
+
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
 		nand-controller@1800 {
 			#address-cells = <1>;
 			#size-cells = <0>;
