From b627cebfc64dd944b9571203e30456efbc0101c3 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Mon, 8 Feb 2021 11:22:01 +0000
Subject: [PATCH] drm/vc4: Register dsi0 as the correct vc4 encoder
 type

vc4_dsi was registering both dsi0 and dsi1 as VC4_ENCODER_TYPE_DSI1
which seemed to work OK for a single DSI display, but fails
if there are two DSI displays connected.

Update to register the correct type.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 drivers/gpu/drm/vc4/vc4_dsi.c | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

--- a/drivers/gpu/drm/vc4/vc4_dsi.c
+++ b/drivers/gpu/drm/vc4/vc4_dsi.c
@@ -1506,7 +1506,8 @@ static int vc4_dsi_bind(struct device *d
 		return -ENOMEM;
 
 	INIT_LIST_HEAD(&dsi->bridge_chain);
-	vc4_dsi_encoder->base.type = VC4_ENCODER_TYPE_DSI1;
+	vc4_dsi_encoder->base.type = dsi->variant->port ?
+			VC4_ENCODER_TYPE_DSI1 : VC4_ENCODER_TYPE_DSI0;
 	vc4_dsi_encoder->dsi = dsi;
 	dsi->encoder = &vc4_dsi_encoder->base.base;
 
