// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca956x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	model = "TP-Link Archer A9 v6";
	compatible = "tplink,archer-a9-v6", "qca,qcn5500", "qca,qca9560";

	aliases {
		label-mac-device = &eth0;
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		wps {
			label = "wps";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "green:power";
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		usb {
			label = "green:usb";
			gpios = <&gpio 0 GPIO_ACTIVE_HIGH>;
			trigger-sources = <&hub_port0>;
			linux,default-trigger = "usbport";
		};

		wan {
			label = "green:wan";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};

		wan_orange {
			label = "orange:wan";
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
		};

		wlan2g {
			label = "green:wlan2g";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		wlan5g {
			label = "green:wlan5g";
			gpios = <&gpio 20 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "phy0tpt";
		};

		wps {
			label = "green:wps";
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
		};
	};
};

&eth0 {
	status = "okay";

	pll-data = <0x03000101 0x00000101 0x00001919>;

	phy-mode = "sgmii";
	phy-handle = <&phy0>;

	nvmem-cells = <&macaddr_info_8>;
	nvmem-cell-names = "mac-address";
};

&mdio0 {
	status = "okay";

	phy-mask = <0>;

	phy0: ethernet-phy@0 {
		reg = <0>;
		phy-mode = "sgmii";
		qca,mib-poll-interval = <500>;

		qca,ar8327-initvals = <
			0x04 0x80080080 /* PORT0 PAD MODE CTRL */
			0x08 0x00000000 /* PORT5 PAD MODE CTRL */
			0x0c 0x00000000 /* PORT6 PAD MODE CTRL */
			0x10 0x00000080 /* POWER_ON_STRAP */
			0x7c 0x0000007e /* PORT0_STATUS */
			0x94 0x00000200 /* PORT6_STATUS */
			>;
	};
};

&pcie {
	status = "okay";

	wifi@0,0 {
		compatible = "pci168c,0046";
		reg = <0 0 0 0 0>;

		nvmem-cells = <&macaddr_info_8>, <&precal_art_5000>;
		nvmem-cell-names = "mac-address", "pre-calibration";

		mac-address-increment = <(-1)>;
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;
		m25p,fast-read;

		mtdparts: partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "factory-uboot";
				reg = <0x000000 0x020000>;
				read-only;
			};

			partition@20000 {
				label = "u-boot";
				reg = <0x020000 0x020000>;
				read-only;
			};

			partition@40000 {
				label = "partition-table";
				reg = <0x040000 0x010000>;
				read-only;
			};

			partition@50000 {
				label = "art";
				reg = <0x050000 0x010000>;
				read-only;

				compatible = "nvmem-cells";
				#address-cells = <1>;
				#size-cells = <1>;

				cal_art_1000: cal@1000 {
					reg = <0x1000 0x440>;
				};

				precal_art_5000: precal@5000 {
					reg = <0x5000 0x2f20>;
				};
			};

			partition@60000 {
				label = "info";
				reg = <0x060000 0x020000>;
				read-only;

				compatible = "nvmem-cells";
				#address-cells = <1>;
				#size-cells = <1>;

				macaddr_info_8: macaddr@8 {
					reg = <0x8 0x6>;
				};
			};

			partition@80000 {
				label = "user-config";
				reg = <0x080000 0x040000>;
				read-only;
			};

			partition@c0000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x0c0000 0xf00000>;
			};

			partition@fc0000 {
				label = "log";
				reg = <0xfc0000 0x020000>;
				read-only;
			};

			partition@fe0000 {
				label = "certificate";
				reg = <0xfe0000 0x010000>;
				read-only;
			};

			partition@ff0000 {
				label = "default-config";
				reg = <0xff0000 0x010000>;
				read-only;
			};
		};
	};
};

&usb_phy0 {
	status = "okay";
};

&usb0 {
	#address-cells = <1>;
	#size-cells = <0>;
	status = "okay";

	hub_port0: port@1 {
		reg = <1>;
		#trigger-source-cells = <0>;
	};
};

&wmac {
	/* TODO: missing support in ath9k */
	status = "disabled";

	nvmem-cells = <&cal_art_1000>, <&macaddr_info_8>;
	nvmem-cell-names = "calibration", "mac-address";
};
