/dts-v1/;

/ {
	#address-cells = <1>;
	#size-cells = <1>;
	compatible = "brcm,bcm63268";

	aliases {
		nflash = &nflash;
		pinctrl = &pinctrl;
		serial0 = &uart0;
		serial1 = &uart1;
		spi0 = &lsspi;
		spi1 = &hsspi;
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu@0 {
			compatible = "brcm,bmips4350", "mips,mips4Kc";
			device_type = "cpu";
			reg = <0>;
		};

		cpu@1 {
			compatible = "brcm,bmips4350", "mips,mips4Kc";
			device_type = "cpu";
			reg = <1>;
		};
	};

	cpu_intc: interrupt-controller {
		#address-cells = <0>;
		compatible = "mti,cpu-interrupt-controller";

		interrupt-controller;
		#interrupt-cells = <1>;
	};

	memory { device_type = "memory"; reg = <0 0>; };

	ubus@10000000 {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;
		compatible = "simple-bus";
		interrupt-parent = <&periph_intc>;

		ext_intc: interrupt-controller@10000018 {
			compatible = "brcm,bcm6345-ext-intc";
			reg = <0x10000018 0x4>;

			interrupt-controller;
			#interrupt-cells = <2>;

			interrupts = <44>, <45>, <46>, <47>;
		};

		periph_intc: interrupt-controller@10000020 {
			compatible = "brcm,bcm6345-l1-intc";
			reg = <0x10000020 0x20>,
			      <0x10000040 0x20>;

			interrupt-controller;
			#interrupt-cells = <1>;

			interrupt-parent = <&cpu_intc>;
			interrupts = <2>, <3>;
		};

		pinctrl: pin-controller@100000c0 {
			compatible = "brcm,bcm63268-pinctrl";
			reg = <0x100000c0 0x8>,
			      <0x100000c8 0x8>,
			      <0x100000d0 0x4>,
			      <0x100000d8 0x4>,
			      <0x100000dc 0x4>,
			      <0x100000f8 0x4>;
			reg-names = "dirout", "dat", "led", "mode",
				    "ctrl", "basemode";

			gpio-controller;
			#gpio-cells = <2>;

			interrupt-parent = <&ext_intc>;
			interrupts = <0 0>, <1 0>, <2 0>, <3 0>;
			interrupt-names = "gpio32", "gpio33", "gpio34", "gpio35";

			pinctrl_serial_led: serial_led {
				pinctrl_serial_led_clk: serial_led_clk {
					function = "serial_led_clk";
					pins = "gpio0";
				};

				pinctrl_serial_led_data: serial_led_data {
					function = "serial_led_data";
					pins = "gpio1";
				};
			};

			pinctrl_hsspi_cs4: hsspi_cs4 {
				function = "hsspi_cs4";
				pins = "gpio16";
			};

			pinctrl_hsspi_cs5: hsspi_cs5 {
				function = "hsspi_cs5";
				pins = "gpio17";
			};

			pinctrl_hsspi_cs6: hsspi_cs6 {
				function = "hsspi_cs6";
				pins = "gpio8";
			};

			pinctrl_hsspi_cs7: hsspi_cs7 {
				function = "hsspi_cs7";
				pins = "gpio9";
			};

			pinctrl_adsl_spi: adsl_spi {
				pinctrl_adsl_spi_miso: adsl_spi_miso {
					function = "adsl_spi_miso";
					pins = "gpio18";
				};

				pinctrl_adsl_spi_mosi: adsl_spi_mosi {
					function = "adsl_spi_mosi";
					pins = "gpio19";
				};
			};

			pinctrl_vreq_clk: vreq_clk {
				function = "vreq_clk";
				pins = "gpio22";
			};

			pinctrl_pcie_clkreq_b: pcie_clkreq_b {
				function = "pcie_clkreq_b";
				pins = "gpio23";
			};

			pinctrl_robosw_led_clk: robosw_led_clk {
				function = "robosw_led_clk";
				pins = "gpio30";
			};

			pinctrl_robosw_led_data: robosw_led_data {
				function = "robosw_led_data";
				pins = "gpio31";
			};

			pinctrl_nand: nand {
				function = "nand";
				group = "nand_grp";
			};

			pinctrl_gpio35_alt: gpio35_alt {
				function = "gpio35_alt";
				pin = "gpio35";
			};

			pinctrl_dectpd: dectpd {
				function = "dectpd";
				group = "dectpd_grp";
			};

			pinctrl_vdsl_phy_override_0: vdsl_phy_override_0 {
				function = "vdsl_phy_override_0";
				group = "vdsl_phy_override_0_grp";
			};

			pinctrl_vdsl_phy_override_1: vdsl_phy_override_1 {
				function = "vdsl_phy_override_1";
				group = "vdsl_phy_override_1_grp";
			};

			pinctrl_vdsl_phy_override_2: vdsl_phy_override_2 {
				function = "vdsl_phy_override_2";
				group = "vdsl_phy_override_2_grp";
			};

			pinctrl_vdsl_phy_override_3: vdsl_phy_override_3 {
				function = "vdsl_phy_override_3";
				group = "vdsl_phy_override_3_grp";
			};

			pinctrl_dsl_gpio8: dsl_gpio8 {
				function = "dsl_gpio8";
				group = "dsl_gpio8";
			};

			pinctrl_dsl_gpio9: dsl_gpio9 {
				function = "dsl_gpio9";
				group = "dsl_gpio9";
			};
		};

		uart0: serial@10000180 {
			compatible = "brcm,bcm6345-uart";
			reg = <0x10000180 0x18>;

			interrupt-parent = <&periph_intc>;
			interrupts = <5>;

			/* clocks = <&periph_clk>; */
			/* clock-names = "refclk"; */

			status = "disabled";
		};

		uart1: serial@100001a0 {
			compatible = "brcm,bcm6345-uart";
			reg = <0x100001a0 0x18>;

			interrupt-parent = <&periph_intc>;
			interrupts = <34>;

			/* clocks = <&periph_clk>; */
			/* clock-names = "refclk"; */

			status = "disabled";
		};

		lsspi: spi@10000800 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "brcm,bcm6358-spi";
			reg = <0x10000800 0x70c>;
			interrupts = <80>;
			/* clocks = <&clkctl 15>; */
		};

		hsspi: spi@10001000 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "brcm,bcm6328-hsspi";
			reg = <0x10001000 0x600>;
			interrupts = <6>;
			/* clocks = <&clkctl 16>; */
		};

		nflash: nand@10000200 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "brcm,nand-bcm6368",
				     "brcm,brcmnand-v4.0",
				     "brcm,brcmnand";
			reg = <0x10000200 0x180>,
			      <0x10000600 0x200>,
			      <0x100000b0 0x10>;
			reg-names = "nand",
				    "nand-cache",
				    "nand-int-base";

			interrupt-parent = <&periph_intc>;
			interrupts = <50>;

			/* clocks = <&clkctl 20>; */

			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_nand>;

			status = "disabled";
		};

		leds: led-controller@10001900 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "brcm,bcm6328-leds";
			reg = <0x10001900 0x24>;
			status = "disabled";
		};
	};
};
