From 760423dfad53877b468490758fe7ea968ded9402 Mon Sep 17 00:00:00 2001
From: ChiYuan Huang <cy_huang@richtek.com>
Date: Wed, 9 Mar 2022 16:01:43 +0800
Subject: [PATCH 2/2] regulator: rt5190a: Add support for Richtek RT5190A PMIC

Add support for Richtek RT5190A PMIC.

Signed-off-by: ChiYuan Huang <cy_huang@richtek.com>
Link: https://lore.kernel.org/r/1646812903-32496-3-git-send-email-u0084500@gmail.com
Signed-off-by: Mark Brown <broonie@kernel.org>
---
 drivers/regulator/Kconfig             |  10 +
 drivers/regulator/Makefile            |   1 +
 drivers/regulator/rt5190a-regulator.c | 513 ++++++++++++++++++++++++++
 3 files changed, 524 insertions(+)
 create mode 100644 drivers/regulator/rt5190a-regulator.c

--- a/drivers/regulator/Kconfig
+++ b/drivers/regulator/Kconfig
@@ -1037,6 +1037,16 @@ config REGULATOR_RT5033
 	  RT5033 PMIC. The device supports multiple regulators like
 	  current source, LDO and Buck.
 
+config REGULATOR_RT5190A
+	tristate "Richtek RT5190A PMIC"
+	depends on I2C
+	select REGMAP_I2C
+	help
+	  This adds support for voltage regulator in Richtek RT5190A PMIC.
+	  It integratas 1 channel buck controller, 3 channels high efficiency
+	  buck converters, 1 LDO, mute AC OFF depop function, with the general
+	  I2C control interface.
+
 config REGULATOR_RT6160
 	tristate "Richtek RT6160 BuckBoost voltage regulator"
 	depends on I2C
--- a/drivers/regulator/Makefile
+++ b/drivers/regulator/Makefile
@@ -125,6 +125,7 @@ obj-$(CONFIG_REGULATOR_ROHM)	+= rohm-reg
 obj-$(CONFIG_REGULATOR_RT4801)	+= rt4801-regulator.o
 obj-$(CONFIG_REGULATOR_RT4831)	+= rt4831-regulator.o
 obj-$(CONFIG_REGULATOR_RT5033)	+= rt5033-regulator.o
+obj-$(CONFIG_REGULATOR_RT5190A) += rt5190a-regulator.o
 obj-$(CONFIG_REGULATOR_RT6160)	+= rt6160-regulator.o
 obj-$(CONFIG_REGULATOR_RT6245)	+= rt6245-regulator.o
 obj-$(CONFIG_REGULATOR_RTMV20)	+= rtmv20-regulator.o
--- /dev/null
+++ b/drivers/regulator/rt5190a-regulator.c
@@ -0,0 +1,513 @@
+// SPDX-License-Identifier: GPL-2.0+
+
+#include <dt-bindings/regulator/richtek,rt5190a-regulator.h>
+#include <linux/bits.h>
+#include <linux/i2c.h>
+#include <linux/interrupt.h>
+#include <linux/kernel.h>
+#include <linux/module.h>
+#include <linux/of.h>
+#include <linux/property.h>
+#include <linux/regmap.h>
+#include <linux/regulator/driver.h>
+#include <linux/regulator/machine.h>
+#include <linux/regulator/of_regulator.h>
+
+#define RT5190A_REG_MANUFACTURE		0x00
+#define RT5190A_REG_BUCK2VSEL		0x04
+#define RT5190A_REG_BUCK3VSEL		0x05
+#define RT5190A_REG_DCDCCNTL		0x06
+#define RT5190A_REG_ENABLE		0x07
+#define RT5190A_REG_DISCHARGE		0x09
+#define RT5190A_REG_PROTMODE		0x0A
+#define RT5190A_REG_MUTECNTL		0x0B
+#define RT5190A_REG_PGSTAT		0x0F
+#define RT5190A_REG_OVINT		0x10
+#define RT5190A_REG_HOTDIEMASK		0x17
+
+#define RT5190A_VSEL_MASK		GENMASK(6, 0)
+#define RT5190A_RID_BITMASK(rid)	BIT(rid + 1)
+#define RT5190A_BUCK1_DISCHG_MASK	GENMASK(1, 0)
+#define RT5190A_BUCK1_DISCHG_ONVAL	0x01
+#define RT5190A_OVERVOLT_MASK		GENMASK(7, 0)
+#define RT5190A_UNDERVOLT_MASK		GENMASK(15, 8)
+#define RT5190A_CH234OT_MASK		BIT(29)
+#define RT5190A_CHIPOT_MASK		BIT(28)
+
+#define RT5190A_BUCK23_MINUV		600000
+#define RT5190A_BUCK23_MAXUV		1400000
+#define RT5190A_BUCK23_STEPUV		10000
+#define RT5190A_BUCK23_STEPNUM		((1400000 - 600000) / 10000 + 1)
+
+enum {
+	RT5190A_IDX_BUCK1 = 0,
+	RT5190A_IDX_BUCK2,
+	RT5190A_IDX_BUCK3,
+	RT5190A_IDX_BUCK4,
+	RT5190A_IDX_LDO,
+	RT5190A_MAX_IDX
+};
+
+struct rt5190a_priv {
+	struct device *dev;
+	struct regmap *regmap;
+	struct regulator_desc rdesc[RT5190A_MAX_IDX];
+	struct regulator_dev *rdev[RT5190A_MAX_IDX];
+};
+
+static int rt5190a_get_error_flags(struct regulator_dev *rdev,
+				   unsigned int *flags)
+{
+	struct regmap *regmap = rdev_get_regmap(rdev);
+	int rid = rdev_get_id(rdev);
+	unsigned int pgood_stat;
+	int ret;
+
+	ret = regmap_read(regmap, RT5190A_REG_PGSTAT, &pgood_stat);
+	if (ret)
+		return ret;
+
+	if (!(pgood_stat & RT5190A_RID_BITMASK(rid)))
+		*flags = REGULATOR_ERROR_FAIL;
+	else
+		*flags = 0;
+
+	return 0;
+}
+
+static int rt5190a_fixed_buck_set_mode(struct regulator_dev *rdev,
+				       unsigned int mode)
+{
+	struct regmap *regmap = rdev_get_regmap(rdev);
+	int rid = rdev_get_id(rdev);
+	unsigned int mask = RT5190A_RID_BITMASK(rid), val;
+
+	switch (mode) {
+	case REGULATOR_MODE_FAST:
+		val = mask;
+		break;
+	case REGULATOR_MODE_NORMAL:
+		val = 0;
+		break;
+	default:
+		return -EINVAL;
+	}
+
+	return regmap_update_bits(regmap, RT5190A_REG_DCDCCNTL, mask, val);
+}
+
+static unsigned int rt5190a_fixed_buck_get_mode(struct regulator_dev *rdev)
+{
+	struct regmap *regmap = rdev_get_regmap(rdev);
+	int rid = rdev_get_id(rdev);
+	unsigned int val;
+	int ret;
+
+	ret = regmap_read(regmap, RT5190A_REG_DCDCCNTL, &val);
+	if (ret) {
+		dev_err(&rdev->dev, "Failed to get mode [%d]\n", ret);
+		return ret;
+	}
+
+	if (val & RT5190A_RID_BITMASK(rid))
+		return REGULATOR_MODE_FAST;
+
+	return REGULATOR_MODE_NORMAL;
+}
+
+static const struct regulator_ops rt5190a_ranged_buck_ops = {
+	.enable	= regulator_enable_regmap,
+	.disable = regulator_disable_regmap,
+	.is_enabled = regulator_is_enabled_regmap,
+	.set_voltage_sel = regulator_set_voltage_sel_regmap,
+	.get_voltage_sel = regulator_get_voltage_sel_regmap,
+	.list_voltage = regulator_list_voltage_linear,
+	.set_active_discharge = regulator_set_active_discharge_regmap,
+	.get_error_flags = rt5190a_get_error_flags,
+};
+
+static const struct regulator_ops rt5190a_fixed_buck_ops = {
+	.enable	= regulator_enable_regmap,
+	.disable = regulator_disable_regmap,
+	.is_enabled = regulator_is_enabled_regmap,
+	.set_active_discharge = regulator_set_active_discharge_regmap,
+	.set_mode = rt5190a_fixed_buck_set_mode,
+	.get_mode = rt5190a_fixed_buck_get_mode,
+	.get_error_flags = rt5190a_get_error_flags,
+};
+
+static const struct regulator_ops rt5190a_fixed_ldo_ops = {
+	.enable	= regulator_enable_regmap,
+	.disable = regulator_disable_regmap,
+	.is_enabled = regulator_is_enabled_regmap,
+	.set_active_discharge = regulator_set_active_discharge_regmap,
+	.get_error_flags = rt5190a_get_error_flags,
+};
+
+static irqreturn_t rt5190a_irq_handler(int irq, void *data)
+{
+	struct rt5190a_priv *priv = data;
+	__le32 raws;
+	unsigned int events, fields;
+	static const struct {
+		unsigned int bitmask;
+		unsigned int report;
+	} event_tbl[] = {
+		{ RT5190A_OVERVOLT_MASK, REGULATOR_ERROR_REGULATION_OUT },
+		{ RT5190A_UNDERVOLT_MASK, REGULATOR_ERROR_UNDER_VOLTAGE }
+	};
+	int i, j, ret;
+
+	ret = regmap_raw_read(priv->regmap, RT5190A_REG_OVINT, &raws,
+			      sizeof(raws));
+	if (ret) {
+		dev_err(priv->dev, "Failed to read events\n");
+		return IRQ_NONE;
+	}
+
+	events = le32_to_cpu(raws);
+
+	ret = regmap_raw_write(priv->regmap, RT5190A_REG_OVINT, &raws,
+			       sizeof(raws));
+	if (ret)
+		dev_err(priv->dev, "Failed to write-clear events\n");
+
+	/* Handle OV,UV events */
+	for (i = 0; i < ARRAY_SIZE(event_tbl); i++) {
+		fields = events & event_tbl[i].bitmask;
+		fields >>= ffs(event_tbl[i].bitmask) - 1;
+
+		for (j = 0; j < RT5190A_MAX_IDX; j++) {
+			if (!(fields & RT5190A_RID_BITMASK(j)))
+				continue;
+
+			regulator_notifier_call_chain(priv->rdev[j],
+						      event_tbl[i].report,
+						      NULL);
+		}
+	}
+
+	/* Handle CH234 OT event */
+	if (events & RT5190A_CH234OT_MASK) {
+		for (j = RT5190A_IDX_BUCK2; j < RT5190A_IDX_LDO; j++) {
+			regulator_notifier_call_chain(priv->rdev[j],
+						      REGULATOR_ERROR_OVER_TEMP,
+						      NULL);
+		}
+	}
+
+	/* Warning if CHIP OT occur */
+	if (events & RT5190A_CHIPOT_MASK)
+		dev_warn(priv->dev, "CHIP overheat\n");
+
+	return IRQ_HANDLED;
+}
+
+static unsigned int rt5190a_of_map_mode(unsigned int mode)
+{
+	switch (mode) {
+	case RT5190A_OPMODE_AUTO:
+		return REGULATOR_MODE_NORMAL;
+	case RT5190A_OPMODE_FPWM:
+		return REGULATOR_MODE_FAST;
+	default:
+		return REGULATOR_MODE_INVALID;
+	}
+}
+
+static int rt5190a_of_parse_cb(struct rt5190a_priv *priv, int rid,
+			       struct of_regulator_match *match)
+{
+	struct regulator_desc *desc = priv->rdesc + rid;
+	struct regulator_init_data *init_data = match->init_data;
+	struct device_node *np = match->of_node;
+	bool latchup_enable;
+	unsigned int mask = RT5190A_RID_BITMASK(rid), val;
+
+	switch (rid) {
+	case RT5190A_IDX_BUCK1:
+	case RT5190A_IDX_BUCK4:
+	case RT5190A_IDX_LDO:
+		init_data->constraints.apply_uV = 0;
+
+		if (init_data->constraints.min_uV ==
+				init_data->constraints.max_uV)
+			desc->fixed_uV = init_data->constraints.min_uV;
+		else {
+			dev_err(priv->dev,
+				"Variable voltage for fixed regulator\n");
+			return -EINVAL;
+		}
+		break;
+	default:
+		break;
+	}
+
+	latchup_enable = of_property_read_bool(np, "richtek,latchup-enable");
+
+	/* latchup: 0, default hiccup: 1 */
+	val = !latchup_enable ? mask : 0;
+
+	return regmap_update_bits(priv->regmap, RT5190A_REG_PROTMODE, mask, val);
+}
+
+static void rt5190a_fillin_regulator_desc(struct regulator_desc *desc, int rid)
+{
+	static const char * const regu_name[] = { "buck1", "buck2",
+						  "buck3", "buck4",
+						  "ldo" };
+	static const char * const supply[] = { NULL, "vin2", "vin3", "vin4",
+					       "vinldo" };
+
+	desc->name = regu_name[rid];
+	desc->supply_name = supply[rid];
+	desc->owner = THIS_MODULE;
+	desc->type = REGULATOR_VOLTAGE;
+	desc->id = rid;
+	desc->enable_reg = RT5190A_REG_ENABLE;
+	desc->enable_mask = RT5190A_RID_BITMASK(rid);
+	desc->active_discharge_reg = RT5190A_REG_DISCHARGE;
+	desc->active_discharge_mask = RT5190A_RID_BITMASK(rid);
+	desc->active_discharge_on = RT5190A_RID_BITMASK(rid);
+
+	switch (rid) {
+	case RT5190A_IDX_BUCK1:
+		desc->active_discharge_mask = RT5190A_BUCK1_DISCHG_MASK;
+		desc->active_discharge_on = RT5190A_BUCK1_DISCHG_ONVAL;
+		desc->n_voltages = 1;
+		desc->ops = &rt5190a_fixed_buck_ops;
+		desc->of_map_mode = rt5190a_of_map_mode;
+		break;
+	case RT5190A_IDX_BUCK2:
+		desc->vsel_reg = RT5190A_REG_BUCK2VSEL;
+		desc->vsel_mask = RT5190A_VSEL_MASK;
+		desc->min_uV = RT5190A_BUCK23_MINUV;
+		desc->uV_step = RT5190A_BUCK23_STEPUV;
+		desc->n_voltages = RT5190A_BUCK23_STEPNUM;
+		desc->ops = &rt5190a_ranged_buck_ops;
+		break;
+	case RT5190A_IDX_BUCK3:
+		desc->vsel_reg = RT5190A_REG_BUCK3VSEL;
+		desc->vsel_mask = RT5190A_VSEL_MASK;
+		desc->min_uV = RT5190A_BUCK23_MINUV;
+		desc->uV_step = RT5190A_BUCK23_STEPUV;
+		desc->n_voltages = RT5190A_BUCK23_STEPNUM;
+		desc->ops = &rt5190a_ranged_buck_ops;
+		break;
+	case RT5190A_IDX_BUCK4:
+		desc->n_voltages = 1;
+		desc->ops = &rt5190a_fixed_buck_ops;
+		desc->of_map_mode = rt5190a_of_map_mode;
+		break;
+	case RT5190A_IDX_LDO:
+		desc->n_voltages = 1;
+		desc->ops = &rt5190a_fixed_ldo_ops;
+		break;
+	}
+}
+
+static struct of_regulator_match rt5190a_regulator_match[] = {
+	{ .name = "buck1", },
+	{ .name = "buck2", },
+	{ .name = "buck3", },
+	{ .name = "buck4", },
+	{ .name = "ldo", }
+};
+
+static int rt5190a_parse_regulator_dt_data(struct rt5190a_priv *priv)
+{
+	struct device_node *regulator_np;
+	struct regulator_desc *reg_desc;
+	struct of_regulator_match *match;
+	int i, ret;
+
+	for (i = 0; i < RT5190A_MAX_IDX; i++) {
+		reg_desc = priv->rdesc + i;
+		match = rt5190a_regulator_match + i;
+
+		rt5190a_fillin_regulator_desc(reg_desc, i);
+
+		match->desc = reg_desc;
+	}
+
+	regulator_np = of_get_child_by_name(priv->dev->of_node, "regulators");
+	if (!regulator_np) {
+		dev_err(priv->dev, "Could not find 'regulators' node\n");
+		return -ENODEV;
+	}
+
+	ret = of_regulator_match(priv->dev, regulator_np,
+				 rt5190a_regulator_match,
+				 ARRAY_SIZE(rt5190a_regulator_match));
+
+	of_node_put(regulator_np);
+
+	if (ret < 0) {
+		dev_err(priv->dev,
+			"Error parsing regulator init data: %d\n", ret);
+		return ret;
+	}
+
+	for (i = 0; i < RT5190A_MAX_IDX; i++) {
+		match = rt5190a_regulator_match + i;
+
+		ret = rt5190a_of_parse_cb(priv, i, match);
+		if (ret) {
+			dev_err(priv->dev, "Failed in [%d] of_parse_cb\n", i);
+			return ret;
+		}
+	}
+
+	return 0;
+}
+
+static const struct reg_sequence rt5190a_init_patch[] = {
+	{ 0x09, 0x3d, },
+	{ 0x0a, 0x3e, },
+	{ 0x0b, 0x01, },
+	{ 0x10, 0xff, },
+	{ 0x11, 0xff, },
+	{ 0x12, 0xff, },
+	{ 0x13, 0xff, },
+	{ 0x14, 0, },
+	{ 0x15, 0, },
+	{ 0x16, 0x3e, },
+	{ 0x17, 0, }
+};
+
+static int rt5190a_device_initialize(struct rt5190a_priv *priv)
+{
+	bool mute_enable;
+	int ret;
+
+	ret = regmap_register_patch(priv->regmap, rt5190a_init_patch,
+				    ARRAY_SIZE(rt5190a_init_patch));
+	if (ret) {
+		dev_err(priv->dev, "Failed to do register patch\n");
+		return ret;
+	}
+
+	mute_enable = device_property_read_bool(priv->dev,
+						"richtek,mute-enable");
+
+	if (mute_enable) {
+		ret = regmap_write(priv->regmap, RT5190A_REG_MUTECNTL, 0x00);
+		if (ret) {
+			dev_err(priv->dev, "Failed to enable mute function\n");
+			return ret;
+		}
+	}
+
+	return 0;
+}
+
+static int rt5190a_device_check(struct rt5190a_priv *priv)
+{
+	u16 devid;
+	int ret;
+
+	ret = regmap_raw_read(priv->regmap, RT5190A_REG_MANUFACTURE, &devid,
+			      sizeof(devid));
+	if (ret)
+		return ret;
+
+	if (devid) {
+		dev_err(priv->dev, "Incorrect device id 0x%04x\n", devid);
+		return -ENODEV;
+	}
+
+	return 0;
+}
+
+static const struct regmap_config rt5190a_regmap_config = {
+	.reg_bits = 8,
+	.val_bits = 8,
+	.max_register = RT5190A_REG_HOTDIEMASK,
+};
+
+static int rt5190a_probe(struct i2c_client *i2c)
+{
+	struct rt5190a_priv *priv;
+	struct regulator_config cfg = {};
+	int i, ret;
+
+	priv = devm_kzalloc(&i2c->dev, sizeof(*priv), GFP_KERNEL);
+	if (!priv)
+		return -ENOMEM;
+
+	priv->dev = &i2c->dev;
+
+	priv->regmap = devm_regmap_init_i2c(i2c, &rt5190a_regmap_config);
+	if (IS_ERR(priv->regmap)) {
+		dev_err(&i2c->dev, "Failed to allocate regmap\n");
+		return PTR_ERR(priv->regmap);
+	}
+
+	ret = rt5190a_device_check(priv);
+	if (ret) {
+		dev_err(&i2c->dev, "Failed to check device %d\n", ret);
+		return ret;
+	}
+
+	ret = rt5190a_device_initialize(priv);
+	if (ret) {
+		dev_err(&i2c->dev, "Failed to initialize the device\n");
+		return ret;
+	}
+
+	ret = rt5190a_parse_regulator_dt_data(priv);
+	if (ret) {
+		dev_err(&i2c->dev, "Failed to parse regulator dt\n");
+		return ret;
+	}
+
+	cfg.dev = &i2c->dev;
+	cfg.regmap = priv->regmap;
+
+	for (i = 0; i < RT5190A_MAX_IDX; i++) {
+		struct regulator_desc *desc = priv->rdesc + i;
+		struct of_regulator_match *match = rt5190a_regulator_match + i;
+
+		cfg.init_data = match->init_data;
+		cfg.of_node = match->of_node;
+
+		priv->rdev[i] = devm_regulator_register(&i2c->dev, desc, &cfg);
+		if (IS_ERR(priv->rdev[i])) {
+			dev_err(&i2c->dev, "Failed to register regulator %s\n",
+				desc->name);
+			return PTR_ERR(priv->rdev[i]);
+		}
+	}
+
+	if (i2c->irq) {
+		ret = devm_request_threaded_irq(&i2c->dev, i2c->irq, NULL,
+						rt5190a_irq_handler,
+						IRQF_ONESHOT,
+						dev_name(&i2c->dev), priv);
+		if (ret) {
+			dev_err(&i2c->dev, "Failed to register interrupt\n");
+			return ret;
+		}
+	}
+
+	return 0;
+}
+
+static const struct of_device_id __maybe_unused rt5190a_device_table[] = {
+	{ .compatible = "richtek,rt5190a", },
+	{}
+};
+MODULE_DEVICE_TABLE(of, rt5190a_device_table);
+
+static struct i2c_driver rt5190a_driver = {
+	.driver = {
+		.name = "rt5190a",
+		.of_match_table = rt5190a_device_table,
+	},
+	.probe_new = rt5190a_probe,
+};
+module_i2c_driver(rt5190a_driver);
+
+MODULE_AUTHOR("ChiYuan Huang <cy_huang@richtek.com>");
+MODULE_DESCRIPTION("Richtek RT5190A Regulator Driver");
+MODULE_LICENSE("GPL v2");
