From 45b575fd9e6a455090820248bf1b98b1f2c7b6c8 Mon Sep 17 00:00:00 2001
From: Lorenzo Bianconi <lorenzo@kernel.org>
Date: Tue, 7 Mar 2023 15:56:00 +0000
Subject: [PATCH 5/7] net: ethernet: mtk_eth_soc: convert caps in mtk_soc_data
 struct to u64

This is a preliminary patch to introduce support for MT7988 SoC.

Signed-off-by: Lorenzo Bianconi <lorenzo@kernel.org>
Signed-off-by: Daniel Golle <daniel@makrotopia.org>
---
 drivers/net/ethernet/mediatek/mtk_eth_path.c | 22 +++----
 drivers/net/ethernet/mediatek/mtk_eth_soc.h  | 62 ++++++++++----------
 2 files changed, 42 insertions(+), 42 deletions(-)

--- a/drivers/net/ethernet/mediatek/mtk_eth_path.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_path.c
@@ -15,10 +15,10 @@
 struct mtk_eth_muxc {
 	const char	*name;
 	int		cap_bit;
-	int		(*set_path)(struct mtk_eth *eth, int path);
+	int		(*set_path)(struct mtk_eth *eth, u64 path);
 };
 
-static const char *mtk_eth_path_name(int path)
+static const char *mtk_eth_path_name(u64 path)
 {
 	switch (path) {
 	case MTK_ETH_PATH_GMAC1_RGMII:
@@ -40,7 +40,7 @@ static const char *mtk_eth_path_name(int
 	}
 }
 
-static int set_mux_gdm1_to_gmac1_esw(struct mtk_eth *eth, int path)
+static int set_mux_gdm1_to_gmac1_esw(struct mtk_eth *eth, u64 path)
 {
 	bool updated = true;
 	u32 val, mask, set;
@@ -71,7 +71,7 @@ static int set_mux_gdm1_to_gmac1_esw(str
 	return 0;
 }
 
-static int set_mux_gmac2_gmac0_to_gephy(struct mtk_eth *eth, int path)
+static int set_mux_gmac2_gmac0_to_gephy(struct mtk_eth *eth, u64 path)
 {
 	unsigned int val = 0;
 	bool updated = true;
@@ -94,7 +94,7 @@ static int set_mux_gmac2_gmac0_to_gephy(
 	return 0;
 }
 
-static int set_mux_u3_gmac2_to_qphy(struct mtk_eth *eth, int path)
+static int set_mux_u3_gmac2_to_qphy(struct mtk_eth *eth, u64 path)
 {
 	unsigned int val = 0, mask = 0, reg = 0;
 	bool updated = true;
@@ -125,7 +125,7 @@ static int set_mux_u3_gmac2_to_qphy(stru
 	return 0;
 }
 
-static int set_mux_gmac1_gmac2_to_sgmii_rgmii(struct mtk_eth *eth, int path)
+static int set_mux_gmac1_gmac2_to_sgmii_rgmii(struct mtk_eth *eth, u64 path)
 {
 	unsigned int val = 0;
 	bool updated = true;
@@ -163,7 +163,7 @@ static int set_mux_gmac1_gmac2_to_sgmii_
 	return 0;
 }
 
-static int set_mux_gmac12_to_gephy_sgmii(struct mtk_eth *eth, int path)
+static int set_mux_gmac12_to_gephy_sgmii(struct mtk_eth *eth, u64 path)
 {
 	unsigned int val = 0;
 	bool updated = true;
@@ -218,7 +218,7 @@ static const struct mtk_eth_muxc mtk_eth
 	},
 };
 
-static int mtk_eth_mux_setup(struct mtk_eth *eth, int path)
+static int mtk_eth_mux_setup(struct mtk_eth *eth, u64 path)
 {
 	int i, err = 0;
 
@@ -249,7 +249,7 @@ out:
 
 int mtk_gmac_sgmii_path_setup(struct mtk_eth *eth, int mac_id)
 {
-	int path;
+	u64 path;
 
 	path = (mac_id == 0) ?  MTK_ETH_PATH_GMAC1_SGMII :
 				MTK_ETH_PATH_GMAC2_SGMII;
@@ -260,7 +260,7 @@ int mtk_gmac_sgmii_path_setup(struct mtk
 
 int mtk_gmac_gephy_path_setup(struct mtk_eth *eth, int mac_id)
 {
-	int path = 0;
+	u64 path = 0;
 
 	if (mac_id == 1)
 		path = MTK_ETH_PATH_GMAC2_GEPHY;
@@ -274,7 +274,7 @@ int mtk_gmac_gephy_path_setup(struct mtk
 
 int mtk_gmac_rgmii_path_setup(struct mtk_eth *eth, int mac_id)
 {
-	int path;
+	u64 path;
 
 	path = (mac_id == 0) ?  MTK_ETH_PATH_GMAC1_RGMII :
 				MTK_ETH_PATH_GMAC2_RGMII;
--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.h
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.h
@@ -878,44 +878,44 @@ enum mkt_eth_capabilities {
 };
 
 /* Supported hardware group on SoCs */
-#define MTK_RGMII		BIT(MTK_RGMII_BIT)
-#define MTK_TRGMII		BIT(MTK_TRGMII_BIT)
-#define MTK_SGMII		BIT(MTK_SGMII_BIT)
-#define MTK_ESW			BIT(MTK_ESW_BIT)
-#define MTK_GEPHY		BIT(MTK_GEPHY_BIT)
-#define MTK_MUX			BIT(MTK_MUX_BIT)
-#define MTK_INFRA		BIT(MTK_INFRA_BIT)
-#define MTK_SHARED_SGMII	BIT(MTK_SHARED_SGMII_BIT)
-#define MTK_HWLRO		BIT(MTK_HWLRO_BIT)
-#define MTK_SHARED_INT		BIT(MTK_SHARED_INT_BIT)
-#define MTK_TRGMII_MT7621_CLK	BIT(MTK_TRGMII_MT7621_CLK_BIT)
-#define MTK_QDMA		BIT(MTK_QDMA_BIT)
-#define MTK_NETSYS_V1		BIT(MTK_NETSYS_V1_BIT)
-#define MTK_NETSYS_V2		BIT(MTK_NETSYS_V2_BIT)
-#define MTK_NETSYS_V3		BIT(MTK_NETSYS_V3_BIT)
-#define MTK_SOC_MT7628		BIT(MTK_SOC_MT7628_BIT)
-#define MTK_RSTCTRL_PPE1	BIT(MTK_RSTCTRL_PPE1_BIT)
-#define MTK_U3_COPHY_V2		BIT(MTK_U3_COPHY_V2_BIT)
+#define MTK_RGMII		BIT_ULL(MTK_RGMII_BIT)
+#define MTK_TRGMII		BIT_ULL(MTK_TRGMII_BIT)
+#define MTK_SGMII		BIT_ULL(MTK_SGMII_BIT)
+#define MTK_ESW			BIT_ULL(MTK_ESW_BIT)
+#define MTK_GEPHY		BIT_ULL(MTK_GEPHY_BIT)
+#define MTK_MUX			BIT_ULL(MTK_MUX_BIT)
+#define MTK_INFRA		BIT_ULL(MTK_INFRA_BIT)
+#define MTK_SHARED_SGMII	BIT_ULL(MTK_SHARED_SGMII_BIT)
+#define MTK_HWLRO		BIT_ULL(MTK_HWLRO_BIT)
+#define MTK_SHARED_INT		BIT_ULL(MTK_SHARED_INT_BIT)
+#define MTK_TRGMII_MT7621_CLK	BIT_ULL(MTK_TRGMII_MT7621_CLK_BIT)
+#define MTK_QDMA		BIT_ULL(MTK_QDMA_BIT)
+#define MTK_NETSYS_V1		BIT_ULL(MTK_NETSYS_V1_BIT)
+#define MTK_NETSYS_V2		BIT_ULL(MTK_NETSYS_V2_BIT)
+#define MTK_NETSYS_V3		BIT_ULL(MTK_NETSYS_V3_BIT)
+#define MTK_SOC_MT7628		BIT_ULL(MTK_SOC_MT7628_BIT)
+#define MTK_RSTCTRL_PPE1	BIT_ULL(MTK_RSTCTRL_PPE1_BIT)
+#define MTK_U3_COPHY_V2		BIT_ULL(MTK_U3_COPHY_V2_BIT)
 
 #define MTK_ETH_MUX_GDM1_TO_GMAC1_ESW		\
-	BIT(MTK_ETH_MUX_GDM1_TO_GMAC1_ESW_BIT)
+	BIT_ULL(MTK_ETH_MUX_GDM1_TO_GMAC1_ESW_BIT)
 #define MTK_ETH_MUX_GMAC2_GMAC0_TO_GEPHY	\
-	BIT(MTK_ETH_MUX_GMAC2_GMAC0_TO_GEPHY_BIT)
+	BIT_ULL(MTK_ETH_MUX_GMAC2_GMAC0_TO_GEPHY_BIT)
 #define MTK_ETH_MUX_U3_GMAC2_TO_QPHY		\
-	BIT(MTK_ETH_MUX_U3_GMAC2_TO_QPHY_BIT)
+	BIT_ULL(MTK_ETH_MUX_U3_GMAC2_TO_QPHY_BIT)
 #define MTK_ETH_MUX_GMAC1_GMAC2_TO_SGMII_RGMII	\
-	BIT(MTK_ETH_MUX_GMAC1_GMAC2_TO_SGMII_RGMII_BIT)
+	BIT_ULL(MTK_ETH_MUX_GMAC1_GMAC2_TO_SGMII_RGMII_BIT)
 #define MTK_ETH_MUX_GMAC12_TO_GEPHY_SGMII	\
-	BIT(MTK_ETH_MUX_GMAC12_TO_GEPHY_SGMII_BIT)
+	BIT_ULL(MTK_ETH_MUX_GMAC12_TO_GEPHY_SGMII_BIT)
 
 /* Supported path present on SoCs */
-#define MTK_ETH_PATH_GMAC1_RGMII	BIT(MTK_ETH_PATH_GMAC1_RGMII_BIT)
-#define MTK_ETH_PATH_GMAC1_TRGMII	BIT(MTK_ETH_PATH_GMAC1_TRGMII_BIT)
-#define MTK_ETH_PATH_GMAC1_SGMII	BIT(MTK_ETH_PATH_GMAC1_SGMII_BIT)
-#define MTK_ETH_PATH_GMAC2_RGMII	BIT(MTK_ETH_PATH_GMAC2_RGMII_BIT)
-#define MTK_ETH_PATH_GMAC2_SGMII	BIT(MTK_ETH_PATH_GMAC2_SGMII_BIT)
-#define MTK_ETH_PATH_GMAC2_GEPHY	BIT(MTK_ETH_PATH_GMAC2_GEPHY_BIT)
-#define MTK_ETH_PATH_GDM1_ESW		BIT(MTK_ETH_PATH_GDM1_ESW_BIT)
+#define MTK_ETH_PATH_GMAC1_RGMII	BIT_ULL(MTK_ETH_PATH_GMAC1_RGMII_BIT)
+#define MTK_ETH_PATH_GMAC1_TRGMII	BIT_ULL(MTK_ETH_PATH_GMAC1_TRGMII_BIT)
+#define MTK_ETH_PATH_GMAC1_SGMII	BIT_ULL(MTK_ETH_PATH_GMAC1_SGMII_BIT)
+#define MTK_ETH_PATH_GMAC2_RGMII	BIT_ULL(MTK_ETH_PATH_GMAC2_RGMII_BIT)
+#define MTK_ETH_PATH_GMAC2_SGMII	BIT_ULL(MTK_ETH_PATH_GMAC2_SGMII_BIT)
+#define MTK_ETH_PATH_GMAC2_GEPHY	BIT_ULL(MTK_ETH_PATH_GMAC2_GEPHY_BIT)
+#define MTK_ETH_PATH_GDM1_ESW		BIT_ULL(MTK_ETH_PATH_GDM1_ESW_BIT)
 
 #define MTK_GMAC1_RGMII		(MTK_ETH_PATH_GMAC1_RGMII | MTK_RGMII)
 #define MTK_GMAC1_TRGMII	(MTK_ETH_PATH_GMAC1_TRGMII | MTK_TRGMII)
@@ -1071,7 +1071,7 @@ struct mtk_reg_map {
 struct mtk_soc_data {
 	const struct mtk_reg_map *reg_map;
 	u32             ana_rgc3;
-	u32		caps;
+	u64		caps;
 	u32		required_clks;
 	bool		required_pctl;
 	u8		offload_version;
