[ "$ACTION" == "add" ] || exit 0

PHYNBR=${DEVPATH##*/phy}

[ -n $PHYNBR ] || exit 0

. /lib/functions.sh
. /lib/functions/system.sh

board=$(board_name)

case "$board" in
	acer,predator-w6)
		key_path="/var/qcidata/data"
		[ "$PHYNBR" = "0" ] && cat $key_path/2gMAC > /sys${DEVPATH}/macaddress
		[ "$PHYNBR" = "1" ] && cat $key_path/6gMAC > /sys${DEVPATH}/macaddress
		[ "$PHYNBR" = "2" ] && cat $key_path/5gMAC > /sys${DEVPATH}/macaddress
		;;
	asus,tuf-ax4200)
		CI_UBIPART="UBI_DEV"
		addr=$(mtd_get_mac_binary_ubi "Factory" 0x4)
		# Originally, phy0 is phy1 mac with LA bit set. However, this would conflict
		# addresses on multiple VIFs with the other radio. Set LA bit and increment
		# mac-address instead.
		[ "$PHYNBR" = "0" ] && macaddr_setbit_la $(macaddr_add $addr 1) > /sys${DEVPATH}/macaddress
		[ "$PHYNBR" = "1" ] && echo "$addr" > /sys${DEVPATH}/macaddress
		;;
	bananapi,bpi-r3)
		addr=$(macaddr_add $(cat /sys/class/net/eth0/address) 2)
		[ "$PHYNBR" = "0" ] && macaddr_unsetbit $addr 6 > /sys${DEVPATH}/macaddress
		[ "$PHYNBR" = "1" ] && macaddr_setbit $addr 6 > /sys${DEVPATH}/macaddress
		;;
	cudy,wr3000-v1)
		addr=$(mtd_get_mac_binary bdinfo 0xde00)
		# Originally, phy0 is phy1 mac with LA bit set. However, this would conflict
		# addresses on multiple VIFs with the other radio. Set LA bit and increment
		# mac-address instead.
		[ "$PHYNBR" = "0" ] && echo "$addr" > /sys${DEVPATH}/macaddress
		[ "$PHYNBR" = "1" ] && macaddr_setbit_la $(macaddr_add $addr 1) > /sys${DEVPATH}/macaddress
		;;
	h3c,magic-nx30-pro)
		addr=$(mtd_get_mac_ascii pdt_data_1 ethaddr)
		[ "$PHYNBR" = "0" ] && macaddr_add $addr 2 > /sys${DEVPATH}/macaddress
		[ "$PHYNBR" = "1" ] && macaddr_add $addr 3 > /sys${DEVPATH}/macaddress
		;;
	mercusys,mr90x-v1)
		addr=$(get_mac_binary "/tmp/tp_data/default-mac" 0)
		[ "$PHYNBR" = "0" ] && echo "$addr" > /sys${DEVPATH}/macaddress
		[ "$PHYNBR" = "1" ] && macaddr_add $addr -1 > /sys${DEVPATH}/macaddress
		;;
	netgear,wax220)
		hw_mac_addr=$(mtd_get_mac_ascii u-boot-env mac)
		[ "$PHYNBR" = "0" ] && macaddr_add $hw_mac_addr 2 > /sys${DEVPATH}/macaddress
		[ "$PHYNBR" = "1" ] && macaddr_add $hw_mac_addr 3 > /sys${DEVPATH}/macaddress
		;;
	qihoo,360t7)
		addr=$(mtd_get_mac_ascii factory lanMac)
		[ "$PHYNBR" = "0" ] && macaddr_add $addr 2 > /sys${DEVPATH}/macaddress
		[ "$PHYNBR" = "1" ] && macaddr_add $addr 3 > /sys${DEVPATH}/macaddress
		;;
	tplink,tl-xdr4288|\
	tplink,tl-xdr6086|\
	tplink,tl-xdr6088)
		[ "$PHYNBR" = "0" ] && get_mac_label > /sys${DEVPATH}/macaddress
		;;
	zyxel,ex5601-t0)
		addr=$(mtd_get_mac_binary "Factory" 0x4)
		[ "$PHYNBR" = "1" ] && macaddr_add $addr 1 > /sys${DEVPATH}/macaddress
		;;
	zyxel,nwa50ax-pro)
		hw_mac_addr="$(mtd_get_mac_binary mrd 0x1fff8)"
		[ "$PHYNBR" = "0" ] && macaddr_add $hw_mac_addr 1 > /sys${DEVPATH}/macaddress
		[ "$PHYNBR" = "1" ] && macaddr_add $hw_mac_addr 2 > /sys${DEVPATH}/macaddress
		;;
esac
