From fd7d9124ffa6761f27747daeea599e0ab874c1fa Mon Sep 17 00:00:00 2001
From: Weijie Gao <weijie.gao@mediatek.com>
Date: Wed, 19 Jul 2023 17:17:54 +0800
Subject: [PATCH 29/29] board: mediatek: add MT7988 reference boards

This patch adds general board files based on MT7988 SoCs.

MT7988 uses one mmc controller for booting from both SD and eMMC,
and the pins of mmc controller booting from SD are also shared with
one of spi controllers.
So two configs are need for these boot types:

1. mt7988_rfb_defconfig - SPI-NOR, SPI-NAND and eMMC
2. mt7988_sd_rfb_defconfig - SPI-NAND and SD

Signed-off-by: Weijie Gao <weijie.gao@mediatek.com>
---
 arch/arm/dts/Makefile              |   2 +
 arch/arm/dts/mt7988-rfb.dts        | 182 +++++++++++++++++++++++++++++
 arch/arm/dts/mt7988-sd-rfb.dts     | 134 +++++++++++++++++++++
 board/mediatek/mt7988/MAINTAINERS  |   7 ++
 board/mediatek/mt7988/Makefile     |   3 +
 board/mediatek/mt7988/mt7988_rfb.c |  10 ++
 configs/mt7988_rfb_defconfig       |  83 +++++++++++++
 configs/mt7988_sd_rfb_defconfig    |  71 +++++++++++
 include/configs/mt7988.h           |  14 +++
 9 files changed, 506 insertions(+)
 create mode 100644 arch/arm/dts/mt7988-rfb.dts
 create mode 100644 arch/arm/dts/mt7988-sd-rfb.dts
 create mode 100644 board/mediatek/mt7988/MAINTAINERS
 create mode 100644 board/mediatek/mt7988/Makefile
 create mode 100644 board/mediatek/mt7988/mt7988_rfb.c
 create mode 100644 configs/mt7988_rfb_defconfig
 create mode 100644 configs/mt7988_sd_rfb_defconfig
 create mode 100644 include/configs/mt7988.h

--- a/arch/arm/dts/Makefile
+++ b/arch/arm/dts/Makefile
@@ -1319,6 +1319,8 @@ dtb-$(CONFIG_ARCH_MEDIATEK) += \
 	mt7986b-sd-rfb.dtb \
 	mt7986a-emmc-rfb.dtb \
 	mt7986b-emmc-rfb.dtb \
+	mt7988-rfb.dtb \
+	mt7988-sd-rfb.dtb \
 	mt8183-pumpkin.dtb \
 	mt8512-bm1-emmc.dtb \
 	mt8516-pumpkin.dtb \
--- /dev/null
+++ b/arch/arm/dts/mt7988-rfb.dts
@@ -0,0 +1,182 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * Copyright (c) 2022 MediaTek Inc.
+ * Author: Sam Shih <sam.shih@mediatek.com>
+ */
+
+/dts-v1/;
+#include "mt7988.dtsi"
+#include <dt-bindings/gpio/gpio.h>
+
+/ {
+	model = "mt7988-rfb";
+	compatible = "mediatek,mt7988-rfb";
+
+	chosen {
+		stdout-path = &uart0;
+	};
+
+	memory@40000000 {
+		device_type = "memory";
+		reg = <0 0x40000000 0 0x10000000>;
+	};
+
+	reg_3p3v: regulator-3p3v {
+		compatible = "regulator-fixed";
+		regulator-name = "fixed-3.3V";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		regulator-boot-on;
+		regulator-always-on;
+	};
+
+	reg_1p8v: regulator-1p8v {
+		compatible = "regulator-fixed";
+		regulator-name = "fixed-1.8V";
+		regulator-min-microvolt = <1800000>;
+		regulator-max-microvolt = <1800000>;
+		regulator-boot-on;
+		regulator-always-on;
+	};
+};
+
+&uart0 {
+	status = "okay";
+};
+
+&i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins>;
+	status = "okay";
+};
+
+&eth {
+	status = "okay";
+	mediatek,gmac-id = <0>;
+	phy-mode = "usxgmii";
+	mediatek,switch = "mt7988";
+
+	fixed-link {
+		speed = <1000>;
+		full-duplex;
+		pause;
+	};
+};
+
+&pinctrl {
+	i2c1_pins: i2c1-pins {
+		mux {
+			function = "i2c";
+			groups = "i2c1_0";
+		};
+	};
+
+	pwm_pins: pwm-pins {
+		mux {
+			function = "pwm";
+			groups = "pwm0", "pwm1", "pwm2", "pwm3", "pwm4",
+				 "pwm5", "pwm6", "pwm7";
+		};
+	};
+
+	spi0_pins: spi0-pins {
+		mux {
+			function = "spi";
+			groups = "spi0", "spi0_wp_hold";
+		};
+	};
+
+	spi2_pins: spi2-pins {
+		mux {
+			function = "spi";
+			groups = "spi2", "spi2_wp_hold";
+		};
+	};
+
+	mmc0_pins_default: mmc0default {
+		mux {
+			function = "flash";
+			groups =  "emmc_51";
+		};
+
+		conf-cmd-dat {
+			pins = "EMMC_DATA_0", "EMMC_DATA_1", "EMMC_DATA_2",
+			       "EMMC_DATA_3", "EMMC_DATA_4", "EMMC_DATA_5",
+			       "EMMC_DATA_6", "EMMC_DATA_7", "EMMC_CMD";
+			input-enable;
+		};
+
+		conf-clk {
+			pins = "EMMC_CK";
+		};
+
+		conf-dsl {
+			pins = "EMMC_DSL";
+		};
+
+		conf-rst {
+			pins = "EMMC_RSTB";
+		};
+	};
+};
+
+&pwm {
+	pinctrl-names = "default";
+	pinctrl-0 = <&pwm_pins>;
+	status = "okay";
+};
+
+&spi0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi0_pins>;
+	#address-cells = <1>;
+	#size-cells = <0>;
+	status = "okay";
+	must_tx;
+	enhance_timing;
+	dma_ext;
+	ipm_design;
+	support_quad;
+	tick_dly = <2>;
+	sample_sel = <0>;
+
+	spi_nand@0 {
+		compatible = "spi-nand";
+		reg = <0>;
+		spi-max-frequency = <52000000>;
+	};
+};
+
+&spi2 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi2_pins>;
+	#address-cells = <1>;
+	#size-cells = <0>;
+	status = "okay";
+	must_tx;
+	enhance_timing;
+	dma_ext;
+	ipm_design;
+	support_quad;
+	tick_dly = <2>;
+	sample_sel = <0>;
+
+	spi_nor@0 {
+		compatible = "jedec,spi-nor";
+		reg = <0>;
+		spi-max-frequency = <52000000>;
+	};
+};
+
+&mmc0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc0_pins_default>;
+	max-frequency = <52000000>;
+	bus-width = <8>;
+	cap-mmc-highspeed;
+	cap-mmc-hw-reset;
+	vmmc-supply = <&reg_3p3v>;
+	vqmmc-supply = <&reg_1p8v>;
+	non-removable;
+	status = "okay";
+};
--- /dev/null
+++ b/arch/arm/dts/mt7988-sd-rfb.dts
@@ -0,0 +1,134 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * Copyright (c) 2022 MediaTek Inc.
+ * Author: Sam Shih <sam.shih@mediatek.com>
+ */
+
+/dts-v1/;
+#include "mt7988.dtsi"
+#include <dt-bindings/gpio/gpio.h>
+
+/ {
+	model = "mt7988-rfb";
+	compatible = "mediatek,mt7988-rfb", "mediatek,mt7988-sd-rfb";
+
+	chosen {
+		stdout-path = &uart0;
+	};
+
+	memory@40000000 {
+		device_type = "memory";
+		reg = <0 0x40000000 0 0x10000000>;
+	};
+
+	reg_3p3v: regulator-3p3v {
+		compatible = "regulator-fixed";
+		regulator-name = "fixed-3.3V";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		regulator-boot-on;
+		regulator-always-on;
+	};
+};
+
+&uart0 {
+	status = "okay";
+};
+
+&i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins>;
+	status = "okay";
+};
+
+&eth {
+	status = "okay";
+	mediatek,gmac-id = <0>;
+	phy-mode = "usxgmii";
+	mediatek,switch = "mt7988";
+
+	fixed-link {
+		speed = <1000>;
+		full-duplex;
+		pause;
+	};
+};
+
+&pinctrl {
+	i2c1_pins: i2c1-pins {
+		mux {
+			function = "i2c";
+			groups = "i2c1_0";
+		};
+	};
+
+	pwm_pins: pwm-pins {
+		mux {
+			function = "pwm";
+			groups = "pwm0", "pwm1", "pwm2", "pwm3", "pwm4",
+				 "pwm5", "pwm6", "pwm7";
+		};
+	};
+
+	spi0_pins: spi0-pins {
+		mux {
+			function = "spi";
+			groups = "spi0", "spi0_wp_hold";
+		};
+	};
+
+	mmc1_pins_default: mmc1default {
+		mux {
+			function = "flash";
+			groups =  "emmc_45";
+		};
+
+		conf-cmd-dat {
+			pins = "SPI2_CSB", "SPI2_MISO", "SPI2_MOSI",
+			       "SPI2_CLK", "SPI2_HOLD";
+			input-enable;
+		};
+
+		conf-clk {
+			pins = "SPI2_WP";
+		};
+	};
+};
+
+&pwm {
+	pinctrl-names = "default";
+	pinctrl-0 = <&pwm_pins>;
+	status = "okay";
+};
+
+&spi0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi0_pins>;
+	#address-cells = <1>;
+	#size-cells = <0>;
+	status = "okay";
+	must_tx;
+	enhance_timing;
+	dma_ext;
+	ipm_design;
+	support_quad;
+	tick_dly = <2>;
+	sample_sel = <0>;
+
+	spi_nand@0 {
+		compatible = "spi-nand";
+		reg = <0>;
+		spi-max-frequency = <52000000>;
+	};
+};
+
+&mmc0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc1_pins_default>;
+	max-frequency = <52000000>;
+	bus-width = <4>;
+	cap-sd-highspeed;
+	vmmc-supply = <&reg_3p3v>;
+	vqmmc-supply = <&reg_3p3v>;
+	status = "okay";
+};
--- /dev/null
+++ b/board/mediatek/mt7988/MAINTAINERS
@@ -0,0 +1,7 @@
+MT7988
+M:	Sam Shih <sam.shih@mediatek.com>
+S:	Maintained
+F:	board/mediatek/mt7988
+F:	include/configs/mt7988.h
+F:	configs/mt7988_rfb_defconfig
+F:	configs/mt7988_sd_rfb_defconfig
--- /dev/null
+++ b/board/mediatek/mt7988/Makefile
@@ -0,0 +1,3 @@
+# SPDX-License-Identifier:	GPL-2.0
+
+obj-y	+= mt7988_rfb.o
--- /dev/null
+++ b/board/mediatek/mt7988/mt7988_rfb.c
@@ -0,0 +1,10 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * Copyright (C) 2022 MediaTek Inc.
+ * Author: Sam Shih <sam.shih@mediatek.com>
+ */
+
+int board_init(void)
+{
+	return 0;
+}
--- /dev/null
+++ b/configs/mt7988_rfb_defconfig
@@ -0,0 +1,83 @@
+CONFIG_ARM=y
+CONFIG_SYS_HAS_NONCACHED_MEMORY=y
+CONFIG_POSITION_INDEPENDENT=y
+CONFIG_ARCH_MEDIATEK=y
+CONFIG_TEXT_BASE=0x41e00000
+CONFIG_SYS_MALLOC_F_LEN=0x4000
+CONFIG_NR_DRAM_BANKS=1
+CONFIG_DEFAULT_DEVICE_TREE="mt7988-rfb"
+CONFIG_SYS_PROMPT="MT7988> "
+CONFIG_TARGET_MT7988=y
+CONFIG_DEBUG_UART_BASE=0x11000000
+CONFIG_DEBUG_UART_CLOCK=40000000
+CONFIG_SYS_LOAD_ADDR=0x46000000
+CONFIG_DEBUG_UART=y
+# CONFIG_AUTOBOOT is not set
+CONFIG_DEFAULT_FDT_FILE="mt7988-rfb"
+CONFIG_LOGLEVEL=7
+CONFIG_LOG=y
+CONFIG_SYS_CBSIZE=512
+CONFIG_SYS_PBSIZE=1049
+# CONFIG_BOOTM_NETBSD is not set
+# CONFIG_BOOTM_PLAN9 is not set
+# CONFIG_BOOTM_RTEMS is not set
+# CONFIG_BOOTM_VXWORKS is not set
+# CONFIG_CMD_ELF is not set
+CONFIG_CMD_CLK=y
+CONFIG_CMD_DM=y
+CONFIG_CMD_GPIO=y
+CONFIG_CMD_PWM=y
+CONFIG_CMD_MMC=y
+CONFIG_CMD_MTD=y
+CONFIG_CMD_PING=y
+CONFIG_CMD_SMC=y
+CONFIG_DOS_PARTITION=y
+CONFIG_EFI_PARTITION=y
+CONFIG_PARTITION_TYPE_GUID=y
+CONFIG_ENV_VARS_UBOOT_RUNTIME_CONFIG=y
+CONFIG_NET_RANDOM_ETHADDR=y
+CONFIG_USE_IPADDR=y
+CONFIG_IPADDR="192.168.1.1"
+CONFIG_USE_NETMASK=y
+CONFIG_NETMASK="255.255.255.0"
+CONFIG_USE_SERVERIP=y
+CONFIG_SERVERIP="192.168.1.2"
+CONFIG_PROT_TCP=y
+CONFIG_REGMAP=y
+CONFIG_SYSCON=y
+CONFIG_CLK=y
+CONFIG_MMC_HS200_SUPPORT=y
+CONFIG_MMC_MTK=y
+CONFIG_MTD=y
+CONFIG_DM_MTD=y
+CONFIG_MTD_SPI_NAND=y
+CONFIG_DM_SPI_FLASH=y
+CONFIG_SPI_FLASH_SFDP_SUPPORT=y
+CONFIG_SPI_FLASH_EON=y
+CONFIG_SPI_FLASH_GIGADEVICE=y
+CONFIG_SPI_FLASH_ISSI=y
+CONFIG_SPI_FLASH_MACRONIX=y
+CONFIG_SPI_FLASH_SPANSION=y
+CONFIG_SPI_FLASH_STMICRO=y
+CONFIG_SPI_FLASH_WINBOND=y
+CONFIG_SPI_FLASH_XMC=y
+CONFIG_SPI_FLASH_XTX=y
+CONFIG_SPI_FLASH_MTD=y
+CONFIG_PHY_FIXED=y
+CONFIG_MEDIATEK_ETH=y
+CONFIG_PINCTRL=y
+CONFIG_PINCONF=y
+CONFIG_PINCTRL_MT7988=y
+CONFIG_POWER_DOMAIN=y
+CONFIG_MTK_POWER_DOMAIN=y
+CONFIG_DM_PWM=y
+CONFIG_PWM_MTK=y
+CONFIG_RAM=y
+CONFIG_DM_SERIAL=y
+CONFIG_MTK_SERIAL=y
+CONFIG_SPI=y
+CONFIG_DM_SPI=y
+CONFIG_MTK_SPIM=y
+CONFIG_LZO=y
+CONFIG_HEXDUMP=y
+# CONFIG_EFI_LOADER is not set
--- /dev/null
+++ b/configs/mt7988_sd_rfb_defconfig
@@ -0,0 +1,71 @@
+CONFIG_ARM=y
+CONFIG_SYS_HAS_NONCACHED_MEMORY=y
+CONFIG_POSITION_INDEPENDENT=y
+CONFIG_ARCH_MEDIATEK=y
+CONFIG_TEXT_BASE=0x41e00000
+CONFIG_SYS_MALLOC_F_LEN=0x4000
+CONFIG_NR_DRAM_BANKS=1
+CONFIG_DEFAULT_DEVICE_TREE="mt7988-sd-rfb"
+CONFIG_SYS_PROMPT="MT7988> "
+CONFIG_TARGET_MT7988=y
+CONFIG_DEBUG_UART_BASE=0x11000000
+CONFIG_DEBUG_UART_CLOCK=40000000
+CONFIG_SYS_LOAD_ADDR=0x46000000
+CONFIG_DEBUG_UART=y
+# CONFIG_AUTOBOOT is not set
+CONFIG_DEFAULT_FDT_FILE="mt7988-sd-rfb"
+CONFIG_LOGLEVEL=7
+CONFIG_LOG=y
+CONFIG_SYS_CBSIZE=512
+CONFIG_SYS_PBSIZE=1049
+# CONFIG_BOOTM_NETBSD is not set
+# CONFIG_BOOTM_PLAN9 is not set
+# CONFIG_BOOTM_RTEMS is not set
+# CONFIG_BOOTM_VXWORKS is not set
+# CONFIG_CMD_ELF is not set
+CONFIG_CMD_CLK=y
+CONFIG_CMD_DM=y
+CONFIG_CMD_GPIO=y
+CONFIG_CMD_PWM=y
+CONFIG_CMD_MMC=y
+CONFIG_CMD_MTD=y
+CONFIG_CMD_PING=y
+CONFIG_CMD_SMC=y
+CONFIG_DOS_PARTITION=y
+CONFIG_EFI_PARTITION=y
+CONFIG_PARTITION_TYPE_GUID=y
+CONFIG_ENV_VARS_UBOOT_RUNTIME_CONFIG=y
+CONFIG_NET_RANDOM_ETHADDR=y
+CONFIG_USE_IPADDR=y
+CONFIG_IPADDR="192.168.1.1"
+CONFIG_USE_NETMASK=y
+CONFIG_NETMASK="255.255.255.0"
+CONFIG_USE_SERVERIP=y
+CONFIG_SERVERIP="192.168.1.2"
+CONFIG_PROT_TCP=y
+CONFIG_REGMAP=y
+CONFIG_SYSCON=y
+CONFIG_CLK=y
+CONFIG_MMC_HS200_SUPPORT=y
+CONFIG_MMC_MTK=y
+CONFIG_MTD=y
+CONFIG_DM_MTD=y
+CONFIG_MTD_SPI_NAND=y
+CONFIG_PHY_FIXED=y
+CONFIG_MEDIATEK_ETH=y
+CONFIG_PINCTRL=y
+CONFIG_PINCONF=y
+CONFIG_PINCTRL_MT7988=y
+CONFIG_POWER_DOMAIN=y
+CONFIG_MTK_POWER_DOMAIN=y
+CONFIG_DM_PWM=y
+CONFIG_PWM_MTK=y
+CONFIG_RAM=y
+CONFIG_DM_SERIAL=y
+CONFIG_MTK_SERIAL=y
+CONFIG_SPI=y
+CONFIG_DM_SPI=y
+CONFIG_MTK_SPIM=y
+CONFIG_LZO=y
+CONFIG_HEXDUMP=y
+# CONFIG_EFI_LOADER is not set
--- /dev/null
+++ b/include/configs/mt7988.h
@@ -0,0 +1,14 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+/*
+ * Configuration for MediaTek MT7988 SoC
+ *
+ * Copyright (C) 2022 MediaTek Inc.
+ * Author: Sam Shih <sam.shih@mediatek.com>
+ */
+
+#ifndef __MT7988_H
+#define __MT7988_H
+
+#define CFG_MAX_MEM_MAPPED		0xC0000000
+
+#endif
