From 43913829405fae8dbc5362e40a2fddf2aac1ca45 Mon Sep 17 00:00:00 2001
From: notro <notro@tronnes.org>
Date: Thu, 10 Jul 2014 13:59:47 +0200
Subject: [PATCH] pinctrl-bcm2835: Set base to 0 give expected gpio
 numbering

Signed-off-by: Noralf Tronnes <notro@tronnes.org>

SQUASH: pinctrl: bcm2835: Set base for bcm2711 GPIO to 0

Without this patch GPIOs don't seem to work properly, primarily
noticeable as broken LEDs.

Squash with "pinctrl-bcm2835: Set base to 0 give expected gpio numbering"

Signed-off-by: Phil Elwell <phil@raspberrypi.com>
---
 drivers/pinctrl/bcm/pinctrl-bcm2835.c | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/drivers/pinctrl/bcm/pinctrl-bcm2835.c
+++ b/drivers/pinctrl/bcm/pinctrl-bcm2835.c
@@ -374,7 +374,7 @@ static const struct gpio_chip bcm2835_gp
 	.get = bcm2835_gpio_get,
 	.set = bcm2835_gpio_set,
 	.set_config = gpiochip_generic_config,
-	.base = -1,
+	.base = 0,
 	.ngpio = BCM2835_NUM_GPIOS,
 	.can_sleep = false,
 	.of_gpio_ranges_fallback = bcm2835_of_gpio_ranges_fallback,
@@ -391,7 +391,7 @@ static const struct gpio_chip bcm2711_gp
 	.get = bcm2835_gpio_get,
 	.set = bcm2835_gpio_set,
 	.set_config = gpiochip_generic_config,
-	.base = -1,
+	.base = 0,
 	.ngpio = BCM2711_NUM_GPIOS,
 	.can_sleep = false,
 	.of_gpio_ranges_fallback = bcm2835_of_gpio_ranges_fallback,
