From 756104b856d4bc3121420af3ced342f5fc2b2123 Mon Sep 17 00:00:00 2001
From: Jia-Wei Chang <jia-wei.chang@mediatek.com>
Date: Fri, 8 Apr 2022 12:58:57 +0800
Subject: [PATCH 02/21] cpufreq: mediatek: Remove unused headers

Remove unused headers.

Signed-off-by: Jia-Wei Chang <jia-wei.chang@mediatek.com>
Reviewed-by: AngeloGioacchino Del Regno <angelogioacchino.delregno@collabora.com>
Signed-off-by: Viresh Kumar <viresh.kumar@linaro.org>
---
 drivers/cpufreq/mediatek-cpufreq.c | 2 --
 1 file changed, 2 deletions(-)

--- a/drivers/cpufreq/mediatek-cpufreq.c
+++ b/drivers/cpufreq/mediatek-cpufreq.c
@@ -13,8 +13,6 @@
 #include <linux/platform_device.h>
 #include <linux/pm_opp.h>
 #include <linux/regulator/consumer.h>
-#include <linux/slab.h>
-#include <linux/thermal.h>
 
 #define MIN_VOLT_SHIFT		(100000)
 #define MAX_VOLT_SHIFT		(200000)
