--- rrdcollect-0.2.9.org/doc/sample-rrdcollect.conf
+++ rrdcollect-0.2.9/doc/sample-rrdcollect.conf
@@ -4,12 +4,12 @@
 # Configuration values:
 
 #step = 60
-#directory = /var/lib/rrdtool
+directory = /var/lib/rrdtool
 #loglevel = LOG_NOTICE
 
 # System statistics:
 file:///proc/stat
-"cpu %d %d %d %d"	stat.rrd:cpu_user,cpu_nice,cpu_system,cpu_idle
+"cpu %d %d %d %d %d %d %d"	stat.rrd:cpu_user,cpu_nice,cpu_system,cpu_idle,cpu_iowait,cpu_irq,cpu_softirq
 "ctxt %u"		stat.rrd:ctxt
 "page %u %u"		stat.rrd:page_in,page_out
 "processes %u"		stat.rrd:processes
@@ -21,15 +21,15 @@
 "Swap: %*d %d %*d"		memory.rrd:swap_used
 
 # S.M.A.R.T. HDD temperature:
-file:///proc/ide/hda/smart_values
-7:"%*04x %*04x %02x%*02x"       temperature.rrd:hda
-file:///proc/ide/hdb/smart_values
-7:"%*04x %*04x %02x%*02x"       temperature.rrd:hdb
+#file:///proc/ide/hda/smart_values
+#7:"%*04x %*04x %02x%*02x"       temperature.rrd:hda
+#file:///proc/ide/hdb/smart_values
+#7:"%*04x %*04x %02x%*02x"       temperature.rrd:hdb
 
 # Net: statistics
 file:///proc/net/dev
 " eth0: %d %d %*d %*d %*d %*d %*d %*d %d %d"	eth0.rrd:bytes_in,pkts_in,bytes_out,pkts_out
-" eth1: %d %d %*d %*d %*d %*d %*d %*d %d %d"	eth1.rrd:bytes_in,pkts_in,bytes_out,pkts_out
+#" eth1: %d %d %*d %*d %*d %*d %*d %*d %d %d"	eth1.rrd:bytes_in,pkts_in,bytes_out,pkts_out
 
 # NEW!
 # exec:/// -- instead of reading from /proc/ file data is read from
@@ -40,5 +40,5 @@
 #
 # To use it, you must compile with --enable-exec
 # Remember, programs run with root permissions.  Use at your own risk.
-exec:///bin/df
-"/dev/hda1 %*d %d %d"	hda1.rrd:used,empty
+#exec:///bin/df
+#"/dev/sda1 %*d %d %d"	sda1.rrd:used,empty
