From 86022438ffeb1b87dfcd018bf477fdbb43076691 Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Wed, 8 May 2013 19:35:33 +0200
Subject: [PATCH] rt2x00: rt2800lib: use the extended EEPROM map for RT3883

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>
---
 drivers/net/wireless/ralink/rt2x00/rt2800lib.c |    3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

--- a/drivers/net/wireless/ralink/rt2x00/rt2800lib.c
+++ b/drivers/net/wireless/ralink/rt2x00/rt2800lib.c
@@ -381,7 +381,8 @@ static unsigned int rt2800_eeprom_word_i
 		      wiphy_name(rt2x00dev->hw->wiphy), word))
 		return 0;
 
-	if (rt2x00_rt(rt2x00dev, RT3593))
+	if (rt2x00_rt(rt2x00dev, RT3593) ||
+	    rt2x00_rt(rt2x00dev, RT3883))
 		map = rt2800_eeprom_map_ext;
 	else
 		map = rt2800_eeprom_map;
