From fa5ad9c025610c22048add2f0ad03f62b6ca1e74 Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Mon, 30 Sep 2013 16:53:33 +0200
Subject: [PATCH] rt2x00: rt2800lib: fix antenna configuration for RT3883

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>
---
 drivers/net/wireless/ralink/rt2x00/rt2800lib.c |    3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

--- a/drivers/net/wireless/ralink/rt2x00/rt2800lib.c
+++ b/drivers/net/wireless/ralink/rt2x00/rt2800lib.c
@@ -2017,7 +2017,8 @@ void rt2800_config_ant(struct rt2x00_dev
 	rt2800_bbp_write(rt2x00dev, 3, r3);
 	rt2800_bbp_write(rt2x00dev, 1, r1);
 
-	if (rt2x00_rt(rt2x00dev, RT3593)) {
+	if (rt2x00_rt(rt2x00dev, RT3593) ||
+	    rt2x00_rt(rt2x00dev, RT3883)) {
 		if (ant->rx_chain_num == 1)
 			rt2800_bbp_write(rt2x00dev, 86, 0x00);
 		else
