From 3f963310151f6e630f94acf73ff44493619038ff Mon Sep 17 00:00:00 2001
From: Sean Wang <sean.wang@mediatek.com>
Date: Wed, 20 Dec 2017 14:42:59 +0800
Subject: [PATCH 173/224] clk: mediatek: fixup test-building of MediaTek clock
 drivers

Let the build system looking into the directiory where the clock drivers
resides for the COMPILE_TEST alternative dependency allows test-building
the drivers.

Signed-off-by: Sean Wang <sean.wang@mediatek.com>
Signed-off-by: Stephen Boyd <sboyd@codeaurora.org>
---
 drivers/clk/Makefile | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/clk/Makefile
+++ b/drivers/clk/Makefile
@@ -67,7 +67,7 @@ obj-$(CONFIG_ARCH_MXC)			+= imx/
 obj-$(CONFIG_MACH_INGENIC)		+= ingenic/
 obj-$(CONFIG_ARCH_KEYSTONE)		+= keystone/
 obj-$(CONFIG_MACH_LOONGSON32)		+= loongson1/
-obj-$(CONFIG_ARCH_MEDIATEK)		+= mediatek/
+obj-y					+= mediatek/
 obj-$(CONFIG_COMMON_CLK_AMLOGIC)	+= meson/
 obj-$(CONFIG_MACH_PIC32)		+= microchip/
 ifeq ($(CONFIG_COMMON_CLK), y)
