From b29e72769f843afeb4585c5310f8bf23c0277daf Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime@cerno.tech>
Date: Fri, 9 Apr 2021 17:31:55 +0200
Subject: [PATCH] drm/vc4: Use the new helpers

We just introduced new helpers, so let's use them.

Signed-off-by: Maxime Ripard <maxime@cerno.tech>
---
 drivers/gpu/drm/vc4/vc4_hdmi.c | 23 ++++-------------------
 1 file changed, 4 insertions(+), 19 deletions(-)

--- a/drivers/gpu/drm/vc4/vc4_hdmi.c
+++ b/drivers/gpu/drm/vc4/vc4_hdmi.c
@@ -224,21 +224,6 @@ static int vc4_hdmi_connector_get_modes(
 	return ret;
 }
 
-static bool hdr_metadata_equal(const struct drm_connector_state *old_state,
-			       const struct drm_connector_state *new_state)
-{
-	struct drm_property_blob *old_blob = old_state->hdr_output_metadata;
-	struct drm_property_blob *new_blob = new_state->hdr_output_metadata;
-
-	if (!old_blob || !new_blob)
-		return old_blob == new_blob;
-
-	if (old_blob->length != new_blob->length)
-		return false;
-
-	return !memcmp(old_blob->data, new_blob->data, old_blob->length);
-}
-
 static int vc4_hdmi_connector_atomic_check(struct drm_connector *connector,
 					  struct drm_atomic_state *state)
 {
@@ -247,12 +232,13 @@ static int vc4_hdmi_connector_atomic_che
 	struct drm_connector_state *new_state =
 		drm_atomic_get_new_connector_state(state, connector);
 	struct drm_crtc *crtc = new_state->crtc;
-	struct drm_crtc_state *crtc_state;
 
 	if (!crtc)
 		return 0;
 
-	if (!hdr_metadata_equal(old_state, new_state)) {
+	if (!drm_connector_atomic_hdr_metadata_equal(old_state, new_state)) {
+		struct drm_crtc_state *crtc_state;
+
 		crtc_state = drm_atomic_get_crtc_state(state, crtc);
 		if (IS_ERR(crtc_state))
 			return PTR_ERR(crtc_state);
@@ -351,8 +337,7 @@ static int vc4_hdmi_connector_init(struc
 	connector->stereo_allowed = 1;
 
 	if (vc4_hdmi->variant->supports_hdr)
-		drm_object_attach_property(&connector->base,
-			connector->dev->mode_config.hdr_output_metadata_property, 0);
+		drm_connector_attach_hdr_output_metadata_property(connector);
 
 	drm_connector_attach_encoder(connector, encoder);
 
