From 6baf7e4abcea6f7ac21eccf072a20078b39d064c Mon Sep 17 00:00:00 2001
From: Robert Marko <robimarko@gmail.com>
Date: Wed, 9 Feb 2022 23:13:26 +0100
Subject: [PATCH] arm64: dts: ipq8074: add label to clocks

Add label to clocks node as that makes it easy to add the NSS fixed
clocks that are required in their DTSI.

Signed-off-by: Robert Marko <robimarko@gmail.com>
---
 arch/arm64/boot/dts/qcom/ipq8074.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm64/boot/dts/qcom/ipq8074.dtsi
+++ b/arch/arm64/boot/dts/qcom/ipq8074.dtsi
@@ -15,7 +15,7 @@
 	compatible = "qcom,ipq8074";
 	interrupt-parent = <&intc>;
 
-	clocks {
+	clocks: clocks {
 		sleep_clk: sleep_clk {
 			compatible = "fixed-clock";
 			clock-frequency = <32768>;
